The Milwaukee 1-1/4 HP Compact Router (model M18 FUEL) delivers performance and precision in a compact design. With a full 1-1/4 maximum horsepower, the M18 FUEL is engineered for a range of precision routing applications. 
The M18 FUEL has a powerful 1-1/4 HP (maximum horsepower) motor with a variable speed control dial (10,000-30,000 RPM) that enables the user to match the speed to the application. Additional performance features include electronic speed control to maintain constant speed under load, and soft start feature for smooth start-ups. The M18 FUEL is double-insulated with a heavy-duty aluminum motor housing for increased durability. 
The M18 FUEL is engineered for precision and includes a smooth rack-and-pinion fine depth adjustment system and easy-to-read depth scales for more precise settings. The quick release cam lock system is designed for easy depth adjustments and base removal/installation, with a high-visibility base design for improved handling and performance. 
Additional