## How can we help you?

# New era. New performance.

## 2.5" SSDs

SATA III 6Gb/s SSD230S

# 2.5" SSDs

## SATA III 6Gb/s SSD230S

Transcend's SATA III 6Gb/s SSD230S uses the latest 3D NAND technology that features vertical, stacked expansion of storage cells. By using high-quality flash memory and enhanced firmware algorithms, the SSD230S delivers greater performance and reliability.

加入購物車

### 3D expansion to break through limits

Unlike planar NAND memory, 3D NAND flash features memory cells stacked vertically in multiple layers. 3D NAND overcomes density limitations of 2D planar NAND, and delivers a higher level of performance and endurance.

### Performance boost for everyday computing

Taking full advantage of the SATA III 6Gb/s interface and built-in SLC caching technology, Transcend's SSD230S achieves exceptional transfer speeds of up to 560MB/s read and 520MB/s write.

### Guaranteed endurance and reliability

Transcend's SSD230S offers great Terabytes Written (TBW) values (up to 2,240 TB) indicating the total amount of data you can write into the drive over its lifetime.

###

#### RAID engine and LDPC coding

Detects and corrects transfer errors to prevent data corruption in TLC-based SSD products

#### Garbage Collection

Relocates existing data to release memory blocks

#### Wear-leveling

Distributes data evenly across memory cells to prolong SSD's lifespan

#### DevSleep

Intelligently shuts down SATA interface when not in use to prolong device's battery life

#### DDR3 DRAM cache

Stores a temporary copy of the most active data to shorten access times

### A better choice than HDD

Solid-state drives dominate the market for PC upgrades because they are faster and lighter than hard disk drives. SSDs also feature less power, create less noise when in operation, and are more shock-resistant than traditional hard drives.

### SSD Scope software

Transcend SSD Scope is advanced, user-friendly software that makes it easy to ensure your Transcend SSD remains healthy, and continues to run fast and error-free by determining the condition and optimizing the performance of your drive.

Learn more

### Guaranteed quality

Transcend’s solid state drives are built to the highest standards and rigorously tested, and offer outstanding quality, performance, and reliability.

### Specifications

#### Appearance
Dimensions | 100 mm x 69.85 mm x 6.8 mm (3.94" x 2.75" x 0.28")
Weight | 53 g (1.87 oz)
#### Storage
Flash Type | 3D NAND flash
Capacity | 128 GB 256 GB 512 GB 1 TB 2 TB 4 TB
#### Operating Environment
Operating Temperature | 0°C (32°F) ~ 70°C (158°F)
Operating Voltage | 5V±5%
#### Performance
Sequential Read/Write (CrystalDiskMark) | TB Up to / MB/s 4 TB Up to 560/520 MB/s 2 TB Up to 560/520 MB/s 1 TB Up to 560/500 MB/s 512 GB Up to 560/500 MB/s 256 GB Up to 530/400 MB/s 128 GB Up to 560/380 MB/s GB Up to / MB/s GB Up to / MB/s
4K Random Read/Write (IOmeter) | TB Up to / IOPS 4 TB Up to 90,000/85,000 IOPS 2 TB Up to 85,000/89,000 IOPS 1 TB Up to 85,000/85,000 IOPS 512 GB Up to 65,000/85,000 IOPS 256 GB Up to 65,000/85,000 IOPS 128 GB Up to 35,000/70,000 IOPS GB Up to / IOPS GB Up to / IOPS
Terabytes Written (TBW) | TB TBW 4 TB 2,240 TBW 2 TB 1,120 TBW 1 TB 560 TBW 512 GB 280 TBW 256 GB 140 TBW 128 GB 70 TBW GB TBW GB TBW
Mean Time Between Failures (MTBF) | 2,000,000 hour(s)
Drive Writes Per Day (DWPD) | 0.3 (5 yrs)
Note | Speed may vary due to host hardware, software, usage, and storage capacity. The workload used to rate DWPD may be different from your actual workload, which may vary due to host hardware, software, usage, and storage capacity. Terabytes Written (TBW) expresses the endurance under the highest capacity. For Mac users please visit our Apple Solutions here.
#### Warranty
Certificate | CE UKCA FCC BSMI KC RCM
Warranty | Five-year Limited Warranty
Warranty Policy | Please click here for more information about the Transcend Warranty Policy. Warranty does not apply when SSD Scope's lifetime indicator displays 0% within the warranty coverage.
#### Package
Package Contents | Full unit
#### System Requirement
Operating System | Microsoft Windows 7 or later Linux Kernel 2.6.31 or later
#### Technology
TRIM & NCQ Command |
S.M.A.R.T. |
DDR3 DRAM Cache |
Advanced Garbage Collection |
DevSleep Mode |
RAID Engine |
LDPC Coding |

See more

### Awards

### Honor Award

MikroBitti
Finland

### Price/ performance Award

Tweaks.pl
Poland

### Excellent Quality Award

Tweaks.pl
Poland

### Cost Effective

ALLSSD
Russia

### Order Information

128GB

- TS128GSSD230S

256GB

- TS256GSSD230S

512GB

- TS512GSSD230S

1TB

- TS1TSSD230S

2TB

- TS2TSSD230S

4TB

- TS4TSSD230S

## Product Sheet

View or download the product sheet for detailed product and ordering information.

## Support

Find drivers, manuals, FAQs, or software updates for your product.

## Recommended Products

2.5” SSD/HDD Enclosure Kit

2.5” SSD/HDD Enclosure

## Explore more

Work From Home Hacks

Get ahead. Up your game.

You have already accepted cookies, but you may still revoke your consent at any time. Please see more details at Cookie Statement. Change Settings

You have already rejected cookies, but you may still give your consent at any time. Please see more details at Cookie Statement. Change Settings

This website uses cookies to collect your information, for improving the service quality. You could click Agree to accept cookies or Disagree to reject cookies. If you reject cookies, some functions of this website may not work properly. You may see more details at Cookie Statement.

Agree Disagree