RV260W
RV260W
RV260W
$299.00
All-in-one Cisco Gateway and access point designed to support LAN and WiFi networks.
 Built-in WiFi 5 AP

  Includes Cisco Network for device management

 Full Gigabit routing

 (4) GbE RJ45 LAN ports

Add to Cart
Installation Guide
Technical Specifications

Mechanical

Dimensions

Ø110 x 184.1 mm (Ø4.3 x 7.3")

Weight

1.1 kg (2.3 lb)

Enclosure material
Polycarbonate

Hardware

Processor

Quad-core Arm® Cortex® A57 at 1.7 GHz

System memory

2 GB DDR RAM

Management interface

Ethernet
Bluetooth

Networking interface

LAN: 
(4) GbE RJ45 ports
WAN: 
(1) GbE RJ45 port

Power method

 Universal AC input, 100—240V AC, 0.6A Max., 50/60 Hz

Power supply

AC/DC, internal, 50W

Supported voltage range

100—240V AC

Max. power consumption

26W

Max. TX power
2.4 GHz
5 GHz

23 dBm
26 dBm

MIMO
2.4 GHz
5 GHz
2 x 2
4 x 4

Throughput rate
2.4 GHz
5 GHz
300 Mbps
1.7 Gbps

Antenna gain
2.4 GHz
5 GHz

3 dBi
4.5 dBi

Antenna

(1) Internal, dual-band, quad-polar