# TD2455

## 24” In-Cell Touch Monitor with USB Type-C Input and Advanced Ergonomics

- Versatile touch applications
- Efficient multitasking
- Touch annotation for presentations
- Accurate yet smooth touch experience
- Comfortable working angles & quickly start your work
- Touch support with Windows, Android, Chrome, Linux and Raspberry Pi

### *Due to a hardware incompatibility with macOS USB stack, TD2455 cannot support touch functions by vTouch temporarily.

Sales Enquiry
Share

### OVERVIEW

With responsive in-cell touch technology and an advanced ergonomic design, the ViewSonic® TD2455 touch monitor delivers hands-on control for more productive workspaces and collaborative classrooms. With high-performance in-cell touch technology, this 24” (23.8” viewable) Full HD display provides smooth and responsive touch tracking, along with amazing screen performance, within a sleek and bezel-less design. USB Type-C connectivity offers a single-cable plug-and-play solution for laptops, while DisplayPort output enables easy screen mirroring or extended desktops ideal for office productivity and podium touch applications such as conference rooms or classrooms. A magnetic stylus pen lets you write or draw on screen, and easily attaches to the display stand for secure storage. So whether used on its own on office desktops, as a presentation station in corporate meeting spaces, or as a front-of-classroom interactive teaching hub, the TD2455 helps to boost efficiency and productivity. *Some laptops may need to enter BIOS mode and change the power management setting to “tap-to-wake”.

## Versatile Touch Applications

Whether used as a check-in kiosk at reception, as a collaboration station with co-workers and colleagues at the office, or as a touch podium for front-facing teaching, this sleek and slim touch display seamlessly integrates into your workflow for boosted efficiency and productivity.
Agile yet Scalable Touch Display

## Efficient Multitasking

With advanced DisplayPort Multi-Stream technology and support for up to 4-screen daisy chaining*, this display can transform into the ultimate touch screen workstation – in mirror and extended modes – for increased productivity. *up to 4 with a PC; up to 3 with a laptop
DisplayPort Multi-Stream Transport (MST)

## Touch Annotation for Presentations

An included stylus pen easily attaches to the magnetic base of the display, and allows you to draw, write notes, or perform other detailed tasks that require more accuracy than your fingertips alone. The pen is especially useful during presentations when the TD2455 is attached to a projector.
Fine Writing Stylus

## Accurate yet Smooth Touch Experience

Powered by in-cell touch technology, the TD2455 offers sensitive yet smooth touch response for detailed content editing with fingertips or the touch pen.
10-Point In-Cell Projected Capacitive (PCAP) Touch Technology

## Quickly Start Your Work

The latest USB Type-C input transforms this display into a powerful hub by enabling easy connectivity to PC, laptop, and Chrome systems. In addition, it delivers charging power, video, and audio over a single cable.
USB Type-C

## Comfortable Working Angles

Designed with an ergonomically advanced dual-hinge stand, this display can be tilted and adjusted to deliver a more comfortable user experience.
Ergonomic Dual-Hinge Design

## Incredible Images, Sleek Design

With high-performance in-cell touch technology, this display provides smooth and responsive touch tracking, along with amazing screen performance, within a sleek and bezel-less design.
In-Cell Projected Capacitive (PCAP) Touch Technology

## Minimal Design Concept

The ergonomic stand features an integrated client mount for quick installation of optional mini PC mount on the back of the display. Cable management features also keep your workspace neat.
Optional Mini PC Mount

## Touch support with Windows, Android, Chrome, Linux and Raspberry Pi

## Extra Features

VESA compatibility, low energy consumption with Energy Star, SuperClear® IPS technology, blue light filter, and flicker-free

## Dimensions & I/O Ports

1. Menu Controls
2. VESA Compatible
   (Wall Mount 100x100mm)
3. Internal Speakers
4. AC IN
5. HDMI
6. DP IN
7. USB Type C
8. DP OUT
   (Output/MST daisy chain)
9. Audio Out
10. USB up stream

## REVIEWS

It's finally worth getting touchy-feely with a Windows 11 desktop PC (feat. Viewsonic TD2455)

Read Review

My New Touch Screen Monitor ? | ViewSonic TD2455 Review | IPS Touch Monitor ? | Tech Unboxing

Read Review

ViewSonic TD2445 Monitor Review

“The ViewSonic TD2445 is an excellent monitor”

Read Review

Tạp chí PCMag

“ViewSonic là thương hiệu màn hình tốt nhất 2020”

Read Review

## SPECIFICATIONS

- Display
  Display Size (in.): 24
  Viewable Area (in.): 23.8
  Panel Type: IPS Technology
  Resolution: 1920 x 1080
  Resolution Type: FHD (Full HD)
  Static Contrast Ratio: 1,000:1 (typ)
  Dynamic Contrast Ratio: 50M:1
  Light Source: LED
  Brightness: 250 cd/m² (typ)
  Colors: 16.7M
  Color Space Support: 8 bit (6 bit + Hi-FRC)
  Aspect Ratio: 16:9
  Response Time (Typical GTG): 6ms
  Response Time (GTG w/OD): 6ms
  Viewing Angles: 178º horizontal, 178º vertical
  Backlight Life (Hours): 30000 Hrs (Min)
  Curvature: Flat
  Refresh Rate (Hz): 60
  Blue Light Filter: Yes
  Flicker-Free: Yes
  Color Gamut: NTSC: 72% size (Typ)
  sRGB: 104% size (Typ)
  Pixel Size: 0.275 mm (H) x 0.275 mm (V)
  Touch Screen: Projected Capacitive, 10-point multi-touch
  Surface Treatment: Anti-Glare, Hard Coating (3H)
- Compatibility
  PC Resolution (max): 1920x1080
  Mac® Resolution (max): 1920x1080
  PC Operating System: Windows 7/8/8.1/10/11 certified; macOS tested
  Mac® Resolution (min): 1920x1080
- Connector
  USB 3.2 Type A Down Stream: 2
  USB 3.2 Type B Up Stream: 1
  USB 3.2 Type C Up Stream; DisplayPort Alt mode : 1 (60W power charger)
  3.5mm Audio Out: 1
  HDMI 1.4: 1
  DisplayPort: 1
  DisplayPort Out: 1
  Power in: 3-pin Socket (IEC C14 / CEE22)

- Audio
  Internal Speakers: 2Watts x2
- Power
  Eco Mode (Conserve): 9.7W
  Eco Mode (optimized): 12.8W
  Consumption (typical): 17.9W
  Consumption (max): 20.4W
  Voltage: AC 100-240V
  Stand-by: 0.3W
  Power Supply: Internal Power Supply
- Additional Hardware
  Kensington Lock Slot: 1
- Controls
  Physical Controls: Key 1 (eye), Key 2, Key 3, Key 4, Key 5, Key 6 (power)
  On Screen Display: Input Select, Audio Adjust, ViewMode, Color Adjust, Manual Image Adjust, Setup Menu
- Operating Conditions
  Temperature: 32°F to 104°F (0°C to 40°C)
  Humidity (non-condensing): 20% to 90%
- Wall Mount
  VESA Compatible: 100 x 100 mm
- Input Signal
  Frequency Horizontal: 15 ~ 82KHz
  Frequency Vertical: 50 ~ 75Hz
- Video Input
  Digital Sync: TMDS - HDMI (v1.4), PCI-E - DisplayPort (v1.2), Micro-Packet - Type C
- Ergonomics
  Tilt (Forward/Back): -5º / 60º
- Weight (imperial)
  Net (lbs): 14.2
  Net Without Stand (lbs): 8.2
  Gross (lbs): 18.6
- Weight (metric)
  Net (kg): 6.4
  Net Without Stand (kg): 3.7
  Gross (kg): 8.4
- Dimensions (imperial) (wxhxd)
  Packaging (in.): 24.3 x 16.3 x 11.2
  Physical (in.): 21.2 x 16.8 x 11.3
  Physical Without Stand (in.): 21.2 x 12.6 x 2
- Dimensions (metric) (wxhxd)
  Packaging (mm): 617 x 415 x 285
  Physical (mm): 539 x 426 x 286
  Physical Without Stand (mm): 539 x 320 x 52
- General
  Regulations: cTUVus, FCC-B, ICES003, Energy Star, EPEAT, CEC, MX-CoC, Mexico Energy, CE, CE EMC, CB, RoHS, ErP, REACH, WEEE, EAC, UkrSEPRO, UKCA, BSMI, RCM, GEMS, KC, K-MEPS, BIS, CCC, China RoHS, China Energy Label, CECP
  PACKAGE CONTENTS: TD2455 x1, 3-pin Plug (IEC C13 / CEE22) x1, DisplayPort Cable (v1.2; Male-Male) x1, USB A/B Cable (v3.2; Male-Male) x1, Quick Start Guide x1, Passive touch pen x1, Passive touch pen head x1
  Recycle/Disposal: Please dispose of in accordance with local, state or federal laws.
  Warranty: *Warranty offered may differ from market to market
  Power Management: Energy Star standards, EPEAT

## SUPPORT & DOWNLOADS

#### Datasheets

TD2455 Datasheet (short version)

#### User Guides

TD2455 User Guide (English) See all languages
TD2455 User Guide (Bahasa Indonesia)TD2455 User Guide (Deutsch)TD2455 User Guide (Español )TD2455 User Guide (Français)TD2455 User Guide (Italiano)TD2455 User Guide (Nederlands)TD2455 User Guide (Norsk)TD2455 User Guide (Português)TD2455 User Guide (Română)TD2455 User Guide (Svenska)TD2455 User Guide (Türkçe)TD2455 User Guide (Česky)TD2455 User Guide (Ελληνικά)TD2455 User Guide (Български)TD2455 User Guide (Русский)TD2455 User Guide (简体中文)TD2455 User Guide (繁體中文)TD2455 User Guide (ﺍﻟﻌﺭﺑﻳﺔ)

#### Driver & Software

Standard Monitor Driver Signed Windows 10 x64 Standard Monitor Driver Signed Windows 10 x86 Standard Monitor Driver Signed Windows 7 Standard Monitor Driver Signed Windows 7 x64 Standard Monitor Driver Signed Windows 8 x64 Standard Monitor Driver Signed Windows 8 x86 Standard Monitor Driver Unsigned Windows Standard Monitor Driver Unsigned Windows x64 Standard_Monitor_Driver_Signed_Win11_x64 ViewSplit Software & User Guide for Windows vTouch Software for macOS

#### Safety Compliance

TD2455 BSMI RoHS

#### Reports

TD2455 Carbon Footprint Report

#### Related FAQ

What Kind of Stylus conductive pen is compatible with ViewSonic Touch Monitors?

##### SELECT YOUR REGION

##### Global

English

##### Americas

United States
Canada
Latin America

##### Europe

Österreich
België (Nederlands)
Belgique (francophone)
Česko
France
Deutschland
Қазақстан
Italia
Luxembourg (français)
Netherlands
Polska
România
Россия
España
Schweiz
Türkiye
Україна
United Kingdom
Europe

##### Asia Pacific & Africa

Australia
Bangladesh
Cambodia
中国
香港 (繁體中文)
Hong Kong (English)
India
Indonesia
Israel
日本
한국
Madagascar
Malaysia
Mauritius
Middle East
Mongolia
Myanmar
Nepal
New Zealand
Pakistan
Philippines
Singapore
Sri Lanka
臺灣
ประเทศไทย
Việt Nam
South Africa
Asia Pacific
Loading...