# Danby 14,000 BTU (10,000 SACC) 3-in-1 Portable AC

SKU: DPA100E5WDB-6 Category: Portable Air Conditioners

- Convenient 3-in-1 design: air conditioner, fan, and dehumidifier
- 14,000 BTU (10,000 SACC) portable air conditioner cools spaces up to 550 square feet
- Powerful 3-speed fan
- R32 refrigerant: environmentally friendly, R32’s GWP (Global Warming Potential) is 3x lower than R410a
- Dehumidifier mode with direct drain for continuous operation
- Electronic controls with LED display, shine through chassis, and remote control
- Auto Restart: unit automatically restarts after a power failure
- 24 hour timer
- Single hose design efficiently exhausts warm and humid air outside
- Reusable, washable air filter
- Easy to move castors and integrated handles for easy room-to-room transport
- 24-month warranty on parts and labor with in-home service

MSRP: $729.99

Out of stock

Compare
Description

Cool down with this 14,000 BTU (10,000 SACC) portable air conditioner by Danby, ideal for cooling spaces up to 550 square feet. To help maximize your comfort, the 3-in-1 design: air conditioner, fan, and dehumidifier helps ensure you feel comfortable no matter the weather outside! The castors make this unit easy to move from room to room, and the single-hose design efficiently exhausts warm and humid air out. In addition, the 24-hour programmable timer allows for better control of when the unit operates, which helps you save on your monthly hydro bill. SACC is short for Seasonally Adjusted Cooling Capacity.

Specifications
Product Dimensions

- Product Width
  17.72"
  45.01 cm
- Product Depth
  15.95"
  40.51 cm
- Product Height
  29.33"
  74.50 cm

Package Dimensions

- Package Width
  19.65"
  49.91 cm
- Package Depth
  18.07"
  45.90 cm
- Package Height
  34.65"
  88.01 cm

Weight

- Product Weight
  81.3 lbs
  36.88 kg
- Package Weight
  85.8 lbs
  38.92 kg

Downloads

- Owners Manual (PDF)
- Energy Guide (PDF)
- Product Specifications (PDF)

Warranty

24 months parts and labor coverage. Installation and/or yearly maintenance (cleaning) are not covered under warranty.

FAQs

#### Q. 1) What are the standard Wattage and amps used?

Information pertaining to watts and camps can be found on the rating plated located on the side of the unit.

#### Q. 2) Can I put an extension on the power cord?

We do not recommend using an extension cord.

#### Q. 3) How do I calculate the square feet of the space I would like to cool?

Square feet is calculated by multiplying the length by the width. For example, a room that is 10 feet long by 25 feet wide is 250 square feet.

#### Q. 4) Where do I drain the water from?

The water drains from the drainage port. If you are not using the continuous drain, the internal pan drains from the bottom outlet. Consult your owner's manual for more information.

#### Q. 5) When do I use the drain hose?

During heat mode, dry mode or continuous draining. Please consult your owner's manuals for more details.

#### Q. 6) Can I put an extension on the exhaust hose/drain hose/power cord?

This is not recommended, as the unit is built to operate using the drain hose/power cord provided.

#### Q. 7) Why does my unit have three draining ports?

Units with three drainage ports are units which also feature heat mode. The bottom drainage port empties the internal pan, the middle port is for continuous drain during heat and the top port is for continuous drain during dry mode. Please consult your owner's manual for more detail.

#### Q. 8) What are the differences between the dual hose model and the single hose?

Dual hose models have an intake and exhaust hose. With single hose models, the hose exhausts and the air that is to be conditioned is taken in from the room through the unit.

#### Q. 9) Can I leave my AC in place through the winter? Will this damage it?

No, this is not recommended. Please bring your AC unit indoors during the winter months.

#### Q. 10) Why does the pan fill up so quickly when I have it on heat mode? Is this normal?

On most models with heat mode, it is advised to use the hose for direct drain. This will ensure the pan does not fill up too quickly.

#### Q. 11) What does automatic mode mean?

When selected, this automatically sets the appropriate option for your room based on the ambient temperature. For example, if it is 15°C outside, the unit would flip to fan mode. If it is set to 30°C, the unit would revert back to cooling mode.

#### Q. 12) How can I prevent heat from escaping from my Danby Portable Air Conditioner hose?

There are a few things to check to ensure this doesn't happen: Ensure that the hose is properly installed at both ends and this should minimize heat escape.Ensure the hose is not over extended. Keep the unit as close the window/patio as possible.Ensure the unit is in an area where it's getting lots of air circulation, which allows the unit to run cooler and results in less heat escaping.If the heat is escaping from the exhaust port then the hose is either restricted or not installed properly.Unfortunately, it is not possible to completely stop all heat loss from escaping.

#### Q. 13) Where do I drain water from?

The water drains from the drainage port. If you are not using the continuous drain, the internal pan drains from the bottom outlet. Consult your owner’s manual for more information. Note: while in Cool mode it is important to not drain the water from the unit as it is designed to use the collected water in the cooling process.

#### Q. 14) When do I use the air exhaust hose?

You should always use it during cooling and heating. In most models it should be removed while using fan and dry mode as it is not required. Please consult your owner’s manuals for more details.

#### Q. 15) What are the portable ac decibel levels?

Danby portable air conditioners have a sound rating from 38 decibels to 56 decibels. The exact decibel range is determined by the model of the unit and the mode (fan, cool or heat if available with the model). Danby also has a patented Silencer Technology available on several models that will keep your home cool and comfortable while operating at a 46 decibel to 49 decibel range.

#### Q. 16) What does automatic mode mean?

When automatic mode is selected, this automatically sets the appropriate option for your room based on the set temperature and the ambient temperature. For example, if it is 15°C outside, the unit would flip to fan mode if the set temperature was above 15. If it is set to 25°C the unit would revert to cooling mode. The unit would not revert to cooling mode unless the temperature outside was over 25.

#### Q. 17) Why is my air conditioner not cooling my entire apartment?

Danby air conditioners are designed to cool a single room and not multiple rooms. Any walls or doors will interfere with the air flow.
Cookies are employed to guarantee the optimal experience on our website. By continuing to browse this site, you are indicating your consent to their use. View Policy
Allow Cookies Reject
Manage consent

#### Privacy Overview

This website uses cookies to improve your experience while you navigate through the website. Out of these, the cookies that are categorized as necessary are stored on your browser as they are essential for the working of basic functionalities of the website. We also use third-party cookies that help us analyze and understand how you use this website. These cookies will be stored in your browser only with your consent. You also have the option to opt-out of these cookies. But opting out of some of these cookies may affect your browsing experience.
Necessary
Necessary
Always Enabled
Necessary cookies are absolutely essential for the website to function properly. These cookies ensure basic functionalities and security features of the website, anonymously.

Cookie | Duration | Description
--- | --- | ---
cookielawinfo-checkbox-analytics | 11 months | This cookie is set by GDPR Cookie Consent plugin. The cookie is used to store the user consent for the cookies in the category "Analytics".
cookielawinfo-checkbox-functional | 11 months | The cookie is set by GDPR cookie consent to record the user consent for the cookies in the category "Functional".
cookielawinfo-checkbox-necessary | 11 months | This cookie is set by GDPR Cookie Consent plugin. The cookies is used to store the user consent for the cookies in the category "Necessary".
cookielawinfo-checkbox-others | 11 months | This cookie is set by GDPR Cookie Consent plugin. The cookie is used to store the user consent for the cookies in the category "Other.
cookielawinfo-checkbox-performance | 11 months | This cookie is set by GDPR Cookie Consent plugin. The cookie is used to store the user consent for the cookies in the category "Performance".
viewed_cookie_policy | 11 months | The cookie is set by the GDPR Cookie Consent plugin and is used to store whether or not user has consented to the use of cookies. It does not store any personal data.

Functional
Functional
Functional cookies help to perform certain functionalities like sharing the content of the website on social media platforms, collect feedbacks, and other third-party features.
Performance
Performance
Performance cookies are used to understand and analyze the key performance indexes of the website which helps in delivering a better user experience for the visitors.
Analytics
Analytics
Analytical cookies are used to understand how visitors interact with the website. These cookies help provide information on metrics the number of visitors, bounce rate, traffic source, etc.
Advertisement
Advertisement
Advertisement cookies are used to provide visitors with relevant ads and marketing campaigns. These cookies track visitors across websites and collect information to provide customized ads.
Others
Others
Other uncategorized cookies are those that are being analyzed and have not been classified into a category as yet.
0

0
Your Cart
Your cart is empty Return to Shop

## Sign up for News, Promos & Giveaways!

- First Name*
- Email*
- Postal Code/Zip*
- State / Province:*