XBU02PT1
36V (18V X2) LXT® Brushless Blower Kit with 4 Batteries (5.0Ah)
XBU02PT1

### 36V (18V X2) LXT® Brushless Blower Kit with 4 Batteries (5.0Ah)

Get up to $300 for qualified California Professional Landscapers

- POWER : BL™ Brushless motor delivers up to 120 MPH air velocity and 473 CFM of air volume
- INNOVATION : Two 18V LXT® Lithium-Ion batteries deliver the power and run time for gas powered demands
- VERSATILITY : 6-stage air velocity/volume selection dial with variable speed control trigger
- CONVENIENCE : Sound pressure rating of 61 dB(A); measured per ANSI B 175.2 standard
- INCLUDES : 4 ea. 18V LXT® 5.0Ah battery and dual port charger

- - Download Image as:
  - - JPG
  - - PNG
  - - TIF

OVERVIEW
APPLICATIONS
FEATURES
PRODUCT VIDEOS
RELATED VIDEOS

- #### LXT® Lithium-Ion

  Tool users who unplug the cord with Makita 18V LXT® experience new levels of convenience, efficiency and productivity. Makita created the 18V Lithium-Ion cordless tool category in 2005, and today it is the world’s largest 18V cordless tool line-up. Makita’s leading technology gives tool users unmatched performance and breadth of line, with innovation in motor and battery technology that is obliterating industry standards – and leaving old thinking behind. With high amp-hour batteries, efficient brushed and brushless motors, and 36V (18V X2) LXT® technology, Makita 18V LXT® tools not only meet corded demands, they can exceed the performance of corded, all while remaining in a single cordless platform powered by the industry's fastest-charging 18V lithium-ion batteries. [Learn More]

- #### Star Protection Computer Controls™

  Makita cordless tools are engineered for industrial applications, and for added protection during the most demanding jobs Makita created STAR Protection Computer Controls™. STAR is communications technology that monitors conditions during use, allowing the tool and battery to exchange data to protect against overloading, overdischarging and overheating. If STAR detects conditions that threaten to overload, overdischarge or overheat the tool or battery, the tool will automatically stop. At that time the user can either restart the tool, change or charge the battery, and put the tool back to work. When you slide a Makita 18V LXT® battery with the STAR symbol onto a Makita tool that has either the STAR symbol or a yellow terminal, you are benefitting from STAR Protection Computer Controls™.

- #### XPT™ Extreme Protection Technology

  When the job takes your Makita tool into harsh conditions, Makita Extreme Protection Technology (XPT™) provides added protection. XPT™ is a series of integrated seals engineered to channel away dust and water for increased durability. Wherever the job takes you, Makita tools equipped with XPT™ are engineered for increased durability and longer tool life.

Landscapers and contractors are demanding more cordless alternatives to gas-powered outdoor power equipment. Makita is meeting demand with an expanding line of cordless OPE that includes the 36V (18V X2) LXT® Brushless Blower. With zero emissions and lower noise, the 18V X2 (36V) Cordless Blower is a welcome solution for clean-up applications. It’s powered by two 18V LXT® batteries for maximum power and run time, but without leaving the 18V battery platform. With the efficient Makita BL™ brushless motor, the blower delivers longer run time, increased power and speed, and longer tool life.

Model XBU02PT1 is a kit and includes the Blower, four fast-charging 18V LXT® Lithium-Ion 5.0Ah batteries and an efficient 18V Dual Port Rapid Optimum Charger.

Makita’s efficient BL™ Brushless motor is electronically controlled to optimize battery energy use for up to 50% longer run time per battery charge than similar non-brushless tools. Electronic controls efficiently use battery energy to match the changing demands of the application for increased power and speed when needed. With no carbon brushes, the Makita BL™ Brushless motor runs cooler and more efficiently for longer life. When powered by two 18V 5.0Ah batteries, the efficient brushless motor delivers up to 28 minutes of run-time on dial setting #3 on a single charge.

The Blower features Makita Extreme Protection Technology (XPT™). XPT™ is a protective seal inside the tool, and is engineered for improved operation in harsh conditions by channeling water and dust from key internal components.

It’s part of Makita’s expanding 18V Lithium-Ion system, the world’s largest cordless tool system powered by 18V Lithium-Ion slide-style batteries. Makita 18V Lithium-Ion batteries have the fastest charge times in their categories, so they spend more time working and less time sitting on the charger.

For improved tool performance and extended battery life, Makita created Star Protection Computer Controls™. Star Protection is communication technology that allows the Star Protection-equipped tool and battery to exchange data in real time and monitor conditions during use to protect against overloading, over-discharging and overheating. For increased versatility, the tool can also be powered by Makita 18V LXT® and Compact Lithium-Ion batteries with the star symbol on the battery indicating Star Protection inside.

- Delivers up to 28 minutes of run time at mid-speed (15,800 RPM) using two 18V LXT® 5.0Ah batteries
- BL™ Brushless motor delivers up to 120 MPH air velocity and 473 CFM of air volume
- Sound pressure rating of 61 dB(A); measured per ANSI B 175.2 standard
- Zero emissions and reduced maintenance; no need for gas or oil
- 6-stage air velocity/volume selection dial with variable speed control trigger
- Two 18V LXT® Lithium-Ion batteries deliver the power and run time for gas powered demands without leaving the 18V LXT® platform
- Compact and ergonomic design at only 36-5/8” long
- Weighs only 9.0 lbs. with batteries for reduced operator fatigue
- Features Extreme Protection Technology (XPT™) which is engineered to provide increased dust and water resistance in harsh job site conditions
- In-line fan design provides better tool balance and improved ergonomics
- 3-stage telescoping long nozzle for user convenience
- Conveniently located hole on housing bottom for easy storage
- Instant start-up; simply load two 18V LXT® batteries and the blower is ready to use
- Lock-on button for continuous operation
- 18V LXT® Lithium-Ion 5.0Ah battery BL1850B features an integrated L.E.D. battery charge level indicator
- 18V LXT® Lithium-Ion 5.0Ah battery BL1850B provides up to 65% more run time per charge compared to 3.0Ah battery BL1830
- 18V LXT® Lithium-Ion 5.0Ah battery BL1850B reaches a full charge in 45 minutes or less
- Dual Port Charger charges two (2) 18V LXT® Lithium-Ion 5.0Ah batteries in only 45 minutes
- The Makita Rapid Optimum Charger communicates with the battery’s built-in chip throughout the charging process to optimize battery life by actively controlling current, voltage and temperature
- Built-in fan circulates air through the battery during the charging process to cool the battery for faster charge time.
- 3-year limited warranty on tool, battery and charger
- Only use genuine Makita batteries and chargers

- (1) 36V (18V X2) LXT® Brushless Blower (XBU02Z)
- (4) 18V LXT® Lithium-Ion 5.0Ah Battery (BL1850B)
- (1) 18V LXT® Lithium-Ion Dual Port Charger (DC18RD)
- (1) 3-Stage Telescoping Blower Nozzle (183R02-0)
- (1) Extension Attachment (197888-8)
- Max. Air Volume : 473 CFM
- Max. Air Velocity : 120 MPH
- No Load Speed (variable speed) : 11,400 - 21,500 RPM
- Battery : 2X 18V LXT® Lithium-Ion
- Sound Pressure (per Ansi B175.2 standard) : 61 dB(A)
- Overall Length : 36-5/8"
- Net Weight (with battery) : 9 lbs.
- Form Factor (LXT) : X2
- Motor Type : Brushless
- Shipping Weight : 22 lbs.
- UPC Code : 088381-852111
- Makita XBU02Z Instruction Manual
- XBU02 Instruction Manual
- Makita XBU02Z Parts Breakdown
- Makita XBU02PT1 New Tool Flyer (English)
Page of Start over
197889-6 Flat End Nozzle 166094-6 Shoulder Strap

You May Also Be Interested In...

Page Of Start over
XBU02Z 36V (18V X2) LXT® Brushless Blower BL1850B 18V LXT® Lithium-Ion 5.0Ah Battery DC18RD 18V LXT® Lithium-Ion Dual Port Charger 183R02-0 3-Stage Telescoping Blower Nozzle 197888-8 Extension Attachment CBU02Z 40V max ConnectX™ Brushless Backpack Blower XBU05Z 18V LXT® Blower XBU02PT 36V (18V X2) LXT® Brushless Blower Kit XBU01PT 36V (18V X2) LXT® Blower Kit XBU04Z 36V (18V X2) LXT® Brushless Blower XBU06Z 18V LXT® Floor Blower XBU04PT 36V (18V X2) LXT® Brushless Blower Kit XBU03Z 18V LXT® Brushless Blower XBU01Z 36V (18V X2) LXT® Blower XBU03SM1 18V LXT® Brushless Blower Kit ADBU05Z Outdoor Adventure™ 18V LXT® Blower XBU04PTV 36V (18V X2) LXT® Brushless Blower Kit with Vacuum Attachment Kit XBU05ST1 18V LXT® Blower Kit XBU07SM1 18V LXT® Brushless Blower / Vacuum Mulcher Kit ADBU05ST1 Outdoor Adventure™ 18V LXT® Blower Kit CBU01Z 40V max ConnectX™ Brushless Blower XBU07Z 18V LXT® Brushless Blower / Vacuum Mulcher XUX02SM1X3 18V LXT Brushless Power Head Kit w/ 13" String Trimmer & Blower Attachments
X
Share your wish list
Don't show again

La página que selecciono por el momento no está disponible en español.

Le gustaría:

¿Proceder con esta página en Inglés?