Boeing 787 Dreamliner
300px
The first All Nippon Airways Boeing 787 (JA801A)
Role | Wide-body jet airliner
National origin | United States
Manufacturer | Boeing Commercial Airplanes
First flight | December 15, 2009
Introduction | October 26, 2011, with All Nippon Airways
Status | In service
Primary users | All Nippon Airways Japan Airlines Ethiopian Airlines See Operators section for others
Produced | c.2006?present
Number built | 87 (November 2012)[1]
Program cost | US$32 billion (Boeing's expenditure)[2]
Unit cost | 787-8: US$206.8?million (2012)[3] 787-9: US$243.6?million (2012)[3]

The Boeing 787 Dreamliner is a long-range, mid-size wide-body, twin-engine jet airliner developed by Boeing Commercial Airplanes. Its variants seat 210 to 290 passengers. Boeing states that it is the company's most fuel-efficient airliner and the world's first major airliner to use composite materials for most of its construction.[4] According to Boeing, the 787 consumes 20% less fuel than the similarly-sized 767.[5] Its distinguishing features include a four-panel windshield, noise-reducing chevrons on its engine nacelles, and a smoother nose contour. The 787 shares a common type rating with the larger 777 twinjet, allowing qualified pilots to operate both models, due to related design features.[6]

The aircraft's initial designation was 7E7, prior to its renaming in January 2005.[7] The first 787 was unveiled in a roll-out ceremony on July 8, 2007, at Boeing's Everett assembly factory, by which time it had reached 677 orders; this is more orders from launch to roll-out than any previous wide-body airliner.[8] By October 2011, the 787 program had logged 873 orders from 57 customers, with ILFC having the largest number on order.[1]

The 787 development and production has involved a large-scale collaboration with numerous suppliers around the globe. Final assembly is at the Boeing Everett Factory in Everett, Washington. Assembly is also taking place at a new factory in North Charleston, South Carolina. Both sites will deliver 787s to airline customers. Originally planned to enter service in May 2008, the project has suffered from multiple delays. The airliner's maiden flight took place on December 15, 2009, and completed flight testing in mid-2011. Final Federal Aviation Administration and European Aviation Safety Agency certification was received in late August 2011 and the first model was delivered in late September 2011. It entered commercial service on October 26, 2011.

## Development[edit]

### Background[edit]

During the late 1990s, Boeing began considering replacement aircraft programs as sales for the 767 and Boeing 747-400 slowed. The company proposed two new aircraft, the 747X, which would have lengthened the 747-400 and improved efficiency, and the Sonic Cruiser, which would have achieved 15% higher speeds (approximately Mach 0.98) while burning fuel at the same rate as the existing 767.[9] Market interest for the 747X was tepid, but the Sonic Cruiser had brighter prospects. Several major airlines in the United States, including Continental Airlines, initially showed enthusiasm for the Sonic Cruiser concept, although they also expressed concerns about the operating cost.[10]

File:Boeing 787 original concept.jpg
Earlier proposed design configuration of the Boeing 7E7.

The global airline market was upended by the September 11, 2001 attacks and increased petroleum prices, making airlines more interested in efficiency than speed. The worst-affected airlines, those in the United States, had been considered the most likely customers of the Sonic Cruiser, and thus Boeing officially cancelled the Sonic Cruiser on December 20, 2002. Changing course, the company announced an alternative product using Sonic Cruiser technology in a more conventional configuration, the 7E7, on January 29, 2003.[4][11] The emphasis on a smaller midsize twinjet rather than a large 747-size aircraft represented a shift from hub-and-spoke theory towards the point-to-point theory,[12] in response to analysis of focus groups.[13]

The replacement for the Sonic Cruiser project was dubbed the "7E7"[14] (with a development code name of "Y2"). Technology from the Sonic Cruiser and 7E7 was to be used as part of Boeing's project to replace its entire airliner product line, an endeavor called the Yellowstone Project (of which the 7E7 became the first stage).[15] Early concept images of the 7E7 included rakish cockpit windows, a dropped nose and a distinctive "shark-fin" tail.[16] The "E" was said to stand for various things, such as "efficiency" or "environmentally friendly"; however, in the end, Boeing claimed that it stood merely for "Eight".[4] In July 2003, a public naming competition was held for the 7E7, for which out of 500,000 votes cast online the winning title was Dreamliner.[17] Other names in the pool included eLiner, Global Cruiser and Stratoclimber.[18]

### Design effort[edit]

On April 26, 2004, Japanese airline All Nippon Airways became the launch customer for the Dreamliner, by announcing a firm order for 50 aircraft with deliveries to begin in late 2008.[19] All Nippon Airways' order was initially specified as 30 787-3, 290?330 seat, one-class domestic aircraft, and 20 787-8, long-haul, 210?250 seat, two-class aircraft for regional international routes such as Tokyo Narita?Beijing. The aircraft would allow All Nippon Airways to open new routes to cities not previously served, such as Denver, Moscow, and New Delhi.[20] The 787-3 and 787-8 were to be the initial variants, with the 787-9 entering service in 2010.[21]

All Nippon Airways launched the 787 Dreamliner program with an order for 50 aircraft in 2004. This aircraft made an emergency landing during a test flight in Texas, on November 9, 2010.

The 787 was designed to become the first production composite airliner, with the fuselage assembled in one-piece composite barrel sections instead of the multiple aluminum sheets and some 50,000 fasteners used on existing aircraft.[22][23] Boeing selected two new engine types to power the 787, the General Electric GEnx and Rolls-Royce Trent 1000.[4] Boeing claimed the 787 would be near to 20 percent more fuel-efficient than the 767,[24] with approximately 40 percent of the efficiency gain from the engines,[25] plus gains from aerodynamic improvements,[26] the increased use of lighter-weight composite materials, and advanced systems.[21] The 787-8 and ?9 were intended to be certified to 330 minute ETOPS capability.[27]

During the design phase, the 787 underwent extensive wind tunnel testing at Boeing's Transonic Wind Tunnel, QinetiQ's five-meter wind tunnel at Farnborough, UK, and NASA Ames Research Center's wind tunnel, as well as at the French aerodynamics research agency, ONERA. The final styling of the aircraft was more conservative than earlier proposals, with the fin, nose, and cockpit windows changed to a more conventional form. By the end of 2004, customer-announced orders and commitments for the 787 reached 237 aircraft.[28] Boeing initially priced the 787-8 variant at US$120?million, a low figure that surprised the industry. In 2007, the list price was US$146?151.5?million for the 787-3, US$157?167?million for the 787-8 and US$189?200?million for the 787-9.[29]

### Manufacturing and suppliers[edit]

After stiff competition, Boeing announced on December 16, 2003, that the 787 would be assembled in its factory in Everett, Washington.[4] Instead of building the complete aircraft from the ground up in the traditional manner, final assembly would employ just 800 to 1,200 people to join completed subassemblies and to integrate systems.[30] Boeing assigned its global subcontractors to do more assembly themselves and deliver completed subassemblies to Boeing for final assembly. This approach was intended to result in a leaner and simpler assembly line and lower inventory,[31] with pre-installed systems reducing final assembly time by three-quarters to three days.[32][33]

Assembly of a "Section 41", the nose section of the Boeing 787

Subcontracted assemblies included wing manufacture (Mitsubishi Heavy Industries, Japan, central wing box)[34] horizontal stabilizers (Alenia Aeronautica, Italy; Korea Aerospace Industries, South Korea);[35] fuselage sections (Global Aeronautica, Italy; Boeing, North Charleston, USA; Kawasaki Heavy Industries, Japan; Spirit AeroSystems, Wichita, USA; Korean Air, South Korea);[36][37][38] passenger doors (Lat?co?re, France); cargo doors, access doors, and crew escape door (Saab AB, Sweden); software development (HCL Enterprise India);[39] floor beams (TAL Manufacturing Solutions Limited, India);[40][41] wiring (Labinal, France);[42] wing-tips, flap support fairings, wheel well bulkhead, and longerons (Korean Air, South Korea);[43] landing gear (Messier-Dowty, UK/France);[44] and power distribution and management systems, air conditioning packs (Hamilton Sundstrand, Connecticut, USA).[42][45] Boeing is considering bringing construction of the 787-9 tail in house; the tail of the 787-8 is currently made by Alenia.[46]

To speed delivery of the 787's major components, Boeing modified four used 747-400s into 747 Dreamlifters to transport 787 wings, fuselage sections, and other smaller parts. Japanese industrial participation was very important to the project, with a 35% work share, the first time Japanese firms had taken a lead role in mass production of Boeing airliner wings, and many of the subcontractors supported and funded by the Japanese government.[47] On April 26, 2006, Japanese manufacturer Toray Industries and Boeing announced a production agreement involving US$6?billion worth of carbon fiber, extending a 2004 contract and aimed at easing production concerns.[4]

### Production and delivery delays[edit]

While Boeing had been working to trim excess weight since assembly of the first airframe began, common for new aircraft in development, the company stated in December 2006 that the first six 787s were overweight, with the first aircraft expected to be 5,000 lb (2,300 kg) heavier than specified. According to International Lease Finance Corporation's (ILFC) Steven Udvar-Hazy, the 787-9's operating empty weight was around 14,000 lb (6,400 kg) overweight.[48] The seventh and subsequent aircraft would be the first optimized 787-8s and were expected to meet all goals, with Boeing working on weight reductions.[49][50] As part of this process, Boeing redesigned some parts and made more use of lighter titanium.[51]

The 787 Dreamliner's first public appearance was webcast live on July 8, 2007.

Boeing had originally planned for a first flight by the end of August 2007 and premiered the first 787 at a rollout ceremony on July 8, 2007, which matches the aircraft's designation in the US-style month-day-year format (7/8/07).[52] However, the aircraft's major systems had not been installed at that time, and many parts were attached with temporary non-aerospace fasteners requiring their later replacement with flight fasteners.[53] Although intended to shorten the production process, 787 subcontractors initially had difficulty completing the extra work, because they could not procure the needed parts, perform the subassembly on schedule, or both, leaving remaining assembly work for Boeing to complete as "traveled work".[54][55][56]

On September 5, Boeing announced a three-month delay, blaming a shortage of fasteners as well as incomplete software.[57] On October 10, 2007, a second three-month delay to the first flight and a six-month delay to first deliveries was announced due to problems with the foreign and domestic supply chain, including an ongoing fastener shortage, the lack of documentation from overseas suppliers, and continuing delays with the flight guidance software.[58][59][60] Less than a week later, Mike Bair, the 787 program manager was replaced.[61] On January 16, 2008, Boeing announced a third three-month delay to the first flight of the 787, citing insufficient progress on "traveled work".[62] On March 28, 2008, in an effort to gain more control over the supply chain, Boeing announced that it planned to buy Vought Aircraft Industries' interest in Global Aeronautica;[63] the company later agreed to also buy Vought's North Charleston, S.C. factory.[64]

On April 9, 2008, Boeing officially announced a fourth delay, shifting the maiden flight to the fourth quarter of 2008, and delaying initial deliveries by around 15 months to the third quarter of 2009. The 787-9 variant was postponed to 2012 and the 787-3 variant was to follow with no firm delivery date.[65] On November 4, 2008, the company announced a fifth delay due to incorrect fastener installation and the Boeing machinists strike, stating that the first test flight would not occur in the fourth quarter of 2008.[66][67] After assessing the 787 program schedule with its suppliers,[68] Boeing confirmed on December 11, 2008 that the first flight would be delayed until the second quarter of 2009.[69]

Airlines such as United Airlines and Air India have stated they want compensation from Boeing for the delays.[70][71] Air India also had very serious issues with their 787 Dreamliner when delivered to them. Frustrated with repeated breakdowns and system failures, their management summoned the Boeing team to India and expressed their anguish to them which they remarked as "Teething Problems" with the aircraft.[72]

### Pre-flight ground testing[edit]

As Boeing worked with its suppliers on early 787 production, the aircraft design had proceeded through a series of test goals. On August 7, 2007, on-time certification of the Rolls-Royce Trent 1000 engine by European and US regulators was received.[73] On August 23, 2007, a crash test involving a vertical drop of a partial composite fuselage section from about 15 ft (4.6 m) onto a 1 in (25 mm)-thick steel plate occurred in Mesa, Arizona;[74][75] the results matched what Boeing's engineers had predicted, allowing modeling of various crash scenarios using computational analysis instead of further physical tests.[76][77] While critics had expressed concerns that a composite fuselage could shatter and burn with toxic fumes during crash landings, Boeing's test data indicated no greater toxicity versus conventional metal airframes.[78][79] The crash test was the third in a series of demonstrations conducted to match FAA requirements, which included additional certification criteria owing to the 787's introduction of wide-scale composite materials.[75]

The first Boeing 787 underwent taxi tests at Paine Field in November and December 2009.

The alternative GE GEnx-1B engine achieved certification on March 31, 2008.[80] On June 20, 2008, the 787 team achieved "Power On" of the first aircraft, powering and testing the aircraft's electrical supply and distribution systems.[81] A non-flight 787 test airframe was built for static testing, and on September 27, 2008, over a period of nearly two hours, the fuselage was successfully tested at 14.9 psi (102.7 kPa) differential, which is 150 percent of the maximum pressure expected in commercial service (i.e., when flying at maximum cruising altitude).[82] In December 2008, the Federal Aviation Administration (FAA) passed the maintenance program for the 787.[83]

On May 3, 2009, the first test 787 was moved to the flight line following extensive factory-testing, including landing gear swings, systems integration verification, and a total run-through of the first flight.[84] On May 4, 2009, a press report indicated a 10?15% range reduction, about 6,900 nmi (12,800?km) instead of the originally promised 7,700 to 8,200 nmi (14,800?15,700?km), for early aircraft that were about 8% overweight. Substantial redesign work was expected to correct this, which would complicate increases in production rates;[85] Boeing stated the early 787-8s would have a range of almost 8,000 nmi (14,800?km).[86] As a result, some airlines reportedly delayed deliveries of 787s in order to take later planes that may be closer to the original estimates.[87] Boeing expected to have the weight issues addressed by the 21st production model.[88]

On June 15, 2009, during the Paris Air Show, Boeing said that the 787 would make its first flight within two weeks. However, on June 23, 2009, Boeing announced that the first flight is postponed "due to a need to reinforce an area within the side-of-body section of the aircraft".[89][90][91] Boeing provided an updated 787 schedule on August 27, 2009, with the first flight planned to occur by the end of 2009 and deliveries to begin at the end of 2010.[92] The company expected to write off US$2.5?billion because it considered the first three Dreamliners built unsellable and suitable only for flight tests.[93] On October 28, 2009, Boeing announced the selection of Charleston, SC as the site for a second 787 production line, after soliciting bids from multiple states including Washington.[94] On December 12, 2009, the first 787 completed high speed taxi tests, the last major step before flight.[95][96][97]

### Flight test program[edit]

The first 787 built taking off on its maiden flight

On December 15, 2009, Boeing conducted the Dreamliner's maiden flight with the first 787-8, originating from Snohomish County Airport in Everett, Washington, at 10:27?am PST,[98] and landing at Boeing Field in King County, Washington, at 1:35?pm PST.[99][100] Originally scheduled for four hours, the test flight was shortened to three hours because of bad weather.[101] Boeing's schedule called for a 9-month flight test campaign (later revised to 8.5 months).[102] The company's previous major aircraft, the 777, took 11 months with nine aircraft, partly to demonstrate 180-min ETOPS, one of its main features.[103]

The 787 flight test program was composed of 6 aircraft, ZA001 through ZA006, four with Rolls-Royce Trent 1000 engines and two with GE GEnx-1B64 engines. The second 787, ZA002 in All Nippon Airways livery, flew to Boeing Field on December 22, 2009, to join the flight test program;[104][105] the third 787, ZA004 joined the test fleet with its first flight on February 24, 2010, followed by ZA003 on March 14, 2010.[106] On March 24, 2010, testing for flutter and ground effects was completed, clearing the aircraft to fly its entire flight envelope.[107] On March 28, 2010, the 787 completed the ultimate wing load test, which requires that the wings of a fully assembled aircraft be loaded to 150% of design limit load and held for 3 seconds. The wings were flexed approximately 25 ft (7.6 m) upward during the test.[108] Unlike past aircraft however, the wings were not tested to failure.[109][110] On April 7, Boeing announced that analysis of the data showed the test was a success.[111]

The first 787 to visit Europe, ZA003 at the 2010 Farnborough Airshow

On April 23, 2010, Boeing delivered the newest 787, ZA003, to the McKinley Climatic Laboratory hangar at Eglin Air Force Base, Florida, for extreme weather testing in temperatures ranging from 115 to −45 ?F[Convert: Unknown unit], and prepare it for takeoff at both temperature extremes.[112] Dreamliner ZA005, the fifth 787 and the first with General Electric GEnx engines began ground engine tests in May 2010.[113] ZA005 made its first flight on June 16, 2010 and joined the flight test program.[114] In June 2010, gaps were discovered in the horizontal stabilizers of test aircraft, due to improperly installed shims; all aircraft produced then were to be inspected and repaired.[115] That same month, a 787 experienced an in-flight lightning strike, allowing engineers the opportunity to examine the aircraft's design tolerances.[116] Since composites can have as little as 1/1,000th the electrical conductivity of aluminum, Boeing engineers had added conductive material to ameliorate potential risks and to meet FAA requirements.[78][117][118] FAA management was also planning to adjust requirements to help the 787 show compliance.[119] Inspections following the 787's first recorded lightning strike showed no damage to the aircraft.[116]

The 787 made its first appearance at an international air show at the Farnborough Airshow, UK, on July 18, 2010.[120] On August 2, a Trent 1000 engine suffered a blowout at Rolls-Royce's test facility during ground testing.[121] The failure caused Boeing to reevaluate its timeline for installing Trent 1000 engines, and on August 27, 2010 the manufacturer confirmed that the first delivery to launch customer All Nippon Airways would be delayed until early 2011.[122][123] That same month, Boeing faced compensation claims from airlines owing to ongoing delivery delays.[124] On September 9, 2010, it was reported that a further two 787s might join the test fleet, making a total of eight flight test aircraft.[125] On September 10, 2010, a partial engine surge or runaway occurred in a Trent engine on ZA001 at Roswell.[126] On October 4, 2010, the sixth 787, ZA006 joined the test program with its first flight.[127]

The third 787 built on static display

On November 5, 2010, it was reported that some early 787 deliveries may be delayed, in one case some three months, to allow for rework to address issues found during flight testing.[128][129] On November 9, 2010, Boeing 787, ZA002 made an emergency landing after smoke and flames were detected in the main cabin during a test flight over Texas. A Boeing spokeswoman said the airliner landed safely and the crew was evacuated after landing at the Laredo International Airport, Texas.[130][131][132] The electrical fire caused some systems to fail before landing.[133] Following this incident, Boeing suspended flight testing on November 10, 2010. Ground testing was performed instead.[134][135] On November 22, 2010, Boeing announced that the in-flight fire can be primarily attributed to foreign object debris (FOD) that was present in the electrical bay.[136] After electrical system and software changes, the 787 resumed company flight testing on December 23, 2010.[137][138]

In January 2011, Boeing announced that the first 787 delivery was rescheduled to the third quarter of 2011 due to software and electrical updates following the in-flight fire.[139][140] On February 24, 2011, Boeing announced that the 787 had completed 80% of the test conditions for Rolls-Royce Trent 1000 engine and 60% of the conditions for the General Electric GEnx-1B engine.[141] On July 4, 2011, All Nippon Airways began a week of airline operations testing using a 787 in Japan.[142] As of August 15, 2011, the 787 test aircraft have flown 4,828 hours in 1,707 flights combined.[106] During testing the 787 has visited 14 countries in Asia, Europe, North America, and South America to test in extreme climates and conditions, and to perform route testing.[143] Boeing completed certification testing for Rolls-Royce powered 787-8s on August 13, 2011.[144] The FAA and European Aviation Safety Agency certified the 787 on August 26, 2011 at a ceremony in Everett, Washington.[145][146]

In April 2012, an All Nippon Airways 787 made a delivery flight from Boeing in Seattle to Tokyo?s Haneda Airport partially using biofuel from cooking oil.[147]

### Service entry and operations[edit]

The 787-8 received FAA and EASA certification on August 21, 2011.

Regulatory certification of the 787 cleared the way for deliveries to begin.[146] With the first deliveries at hand, Boeing began preparations to increase 787 production rates from two to ten aircraft per month over the next two years.[146] Production is taking place at assembly lines in Everett and Charleston. The Charleston site's contributions have been clouded by legal difficulties; on April 20, 2011, the National Labor Relations Board alleged that Boeing's second production line in South Carolina violated two sections of the National Labor Relations Act.[94] This labor dispute ended in December 2011 when the National Labor Relations Board dropped its lawsuit after the Machinists union withdrew its complaint as part of a new contract with Boeing.[148] The first 787 assembled at the South Carolina facility was rolled out on April 27, 2012.[149]

The first 787 was officially delivered to All Nippon Airways on September 25, 2011, at Boeing's facilities in Everett, Washington. A ceremony to mark the occasion was also held the next day.[150][151] On September 27, the Dreamliner flew to Haneda Airport.[152][153] The airline took delivery of the second 787 on October 13, 2011.[154]

On October 26, 2011, the 787 flew its first commercial flight from Narita to Hong Kong on All Nippon Airways.[155] The airliner was planned to enter service some three years prior. Tickets for the flight were sold in an online auction, with the highest bidder paying $34,000 for a seat.[156] ANA expects to take delivery of 7 Dreamliners by the end of 2011 and 9 by March 2012.[155] The 787 flew its first commercial long-haul flight on January 21, 2012 from Haneda to Frankfurt on All Nippon Airways.[157]

On December 6, 2011, test aircraft ZA006 (sixth 787 built), powered by General Electric GEnx engines, flew 10,710 nautical miles (19,830 km) non-stop from Boeing Field eastward to Shahjalal International Airport in Dhaka, Bangladesh, setting a new world distance record for aircraft in the 787's weight class, which is between 440,000 pounds (200,000 kg) and 550,000 pounds (250,000 kg). This flight surpassed the previous record of 9,127 nautical miles (16,903 km), set in 2002 by an Airbus A330. The Dreamliner then continued eastbound from Dhaka to return to Boeing Field, setting a world-circling speed record of 42 hours, 27 minutes.[158]

In late 2011, Boeing began a 787 world tour to promote the airliner. It has visited cities in China, Africa, the Middle East, Europe, United States, and others.[159][160][161]

Data from ANA reported that the 787 surpasses the 20% fuel burn reduction promised by Boeing as compared to the 767. On the Tokyo-Frankfurt route the fuel savings was 21%.[162] As part of this report the passenger experience was also rated. Nine in ten passengers said it surpassed their expectations and a quarter said they would go out of their way to fly the 787 again. Air quality and cabin pressure met or exceeded expectations for nine in ten passengers, and 92% of passengers reported that the cabin ambience was as good or better than they expected. Higher humidity levels in the cabin met or exceeded expectations for four in five passengers. Four in ten said headroom was better than expected. Finally, the large windows met or surpassed expectations of 90% of passengers. ANA surveyed 800 passengers who flew the 787 from Tokyo to Frankfurt.[163]

Qatar Airways placed its first 787 on display at the Farnborough Airshow in July 2012. The airline was to officially receive the aircraft in August.[164]

On September 15, 2012, the NTSB requested the grounding of certain 787s due to GE engine failures; GE believes the production problem has already been fixed.[165]

On November 25, 2012, it was reported that Air India had requested a team of Boeing engineers come to India to address issues described as "teething problems" with its aircraft.[166]

## Design[edit]

A near-planform view of a Boeing 787-8 (ZA005) taking off from Boeing Field.

The 787's design features lighter-weight construction. The aircraft is 80% composite by volume.[167] Its materials, listed by weight, are 50% composite, 20% aluminum, 15% titanium, 10% steel, and 5% other.[168][169] Aluminum is used on wing and tail leading edges, titanium used mainly on engines and fasteners, with steel used in various places.[169]

External features include raked wingtips and engine nacelles with noise-reducing serrated edges.[170] The longest-range 787 variant can fly 8,000 to 8,500 nautical miles (15,000 to 15,700 km), enough to cover the Los Angeles to Bangkok or New York City to Hong Kong routes. It has a cruising airspeed of Mach 0.85[171] (561?mph, 903?km/h at typical cruise altitudes).

### Flight systems[edit]

Among 787 flight systems, the most notable contribution to efficiency is the new electrical architecture, which replaces bleed air and hydraulic power sources with electrically powered compressors and pumps, as well as completely eliminating pneumatics and hydraulics from some subsystems (e.g., engine starters or brakes).[172] Another new system is a wing ice protection system that uses electro-thermal heater mats on the wing slats instead of hot bleed air that has been traditionally used.[173][174] An active gust alleviation system, similar to the system used on the B-2 bomber, improves ride quality during turbulence.[175][176]

Boeing 787 flight deck

The 787 flight deck features LCD multi-function displays, all of which will use an industry standard GUI widget toolkit (Cockpit Display System Interfaces to User Systems / ARINC 661).[177] The 787 flight deck includes two head-up displays (HUDs) as a standard feature.[178] Like other Boeing airliners, the 787 will use a yoke instead of a side-stick. The future integration of forward looking infrared into the HUD system for thermal sensing so the pilots can "see" through the clouds is under consideration.[4] The Lockheed Martin Orion spacecraft will use a glass cockpit derived from Honeywell International's 787 flight deck systems.[179]

On the 787, Honeywell and Rockwell Collins provide flight control, guidance, and other avionics systems, including standard dual head up guidance systems,[4] while Thales supplies the integrated standby flight display and electrical power conversion system.[4] A version of Ethernet (Avionics Full-Duplex Switched Ethernet (AFDX) / ARINC 664) will be used to transmit data between the flight deck and aircraft systems.[180] The airplane's control, navigation, and communication systems are networked with the passenger cabin's in-flight internet systems.[181] In January 2008, FAA concerns regarding possible intentional or unintentional passenger access to the 787's computer networks were reported. Boeing responded by stating that various hardware and software solutions are employed to protect the airplane systems, including air gaps in places to physically separate the networks, and firewalls for software separation.[181][182] These measures prevent data transfer from the passenger internet system to the maintenance or navigation systems.[181]

### Composite materials[edit]

Disassembled composite fuselage section of the Boeing 787

Each 787 contains approximately 35 short tons (32,000 kg) of carbon fiber reinforced plastic (CFRP), made with 23 tons of carbon fiber.[183] Carbon fiber composites have a higher strength-to-weight ratio than traditional aircraft materials, and help make the 787 a lighter aircraft.[169] Composites are used on fuselage, wings, tail, doors, and interior. Boeing had built and tested the first commercial aircraft composite section while studying the proposed Sonic Cruiser nearly five years before;[184][185] the Bell Boeing V-22 Osprey military transport uses 50% composites,[186] and the company's C-17 transport has over 16,000 lb (7,300 kg) of structural composites.[187]

Carbon fiber, unlike metal, does not visibly show cracks and fatigue, prompting concerns about the safety risks of widespread use of the material;[78][188][189] the rival Airbus A350 was later announced to be using composite panels on a frame, a more traditional approach, which its contractors regarded as less risky.[79] In addition, the porous properties of composite materials, which may cause delamination as collected moisture expands with altitude, is a potential issue.[190] Boeing has responded by noting that composites have been used on wings and other passenger aircraft parts for many years without incident, and that special defect detection procedures will be instituted for the 787 to detect any potential hidden damage.[191]

In 2006, Boeing launched the 787 GoldCare program.[192] This is an optional, comprehensive life-cycle management service whereby aircraft in the program are routinely monitored and repaired as needed. This is the first program of its kind from Boeing. Post-sale protection programs are not new, but have usually been offered by third party service centers. Boeing is also designing and testing composite hardware so inspections are mainly visual. This will reduce the need for ultrasonic and other non-visual inspection methods, saving time and money.[193]

### Engines[edit]

The toothed exhaust duct covers on the first 787, shown here with thrust-reversers deployed

The 787 features two engines; these engines use all-electrical bleedless systems, eliminating the superheated air conduits normally used for aircraft power, de-icing, and other functions.[4] As part of its "Quiet Technology Demonstrator 2" project, Boeing adopted several engine noise-reducing technologies for the 787. Among these are a redesigned air inlet containing sound-absorbing materials and redesigned exhaust duct covers whose rims are tipped in a toothed or chevron pattern to allow for quieter mixing of exhaust and outside air.[170] Boeing expects these developments to make the 787 significantly quieter both inside and out.[194] The noise-reducing measures ensure that sounds above 85 decibels do not leave airport boundaries.[169]

The two different engine models compatible with the 787 use a standard electrical interface to allow an aircraft to be fitted with either Rolls-Royce Trent 1000 or General Electric GEnx engines. This aims to save time and cost when changing engine types; while previous aircraft can have engines changed to those of a different manufacturer, the high cost and time required makes it rare.[195][196] In 2006, Boeing addressed reports of an extended change period by stating that the 787 engine swap was intended to take 24 hours;[196] engine interchangeability, it is reported, makes the 787 a more flexible asset to airlines, allowing them to change easily from one manufacturer's engine to the other if required.[4]

### Interior[edit]

ANA's first 787 Dreamliner features 2?4?2 economy class seating.

The 787-8 is designed to typically seat 234 passengers in a three-class setup, 240 in two-class domestic configuration, and 296 passengers in a high-density economy arrangement. Seat rows can be arranged in four to six abreast in first or business (e.g., 1?2?1, 2?2?2), with eight or nine abreast in economy (e.g., 3?2?3, 2?4?2, 3?3?3). Typical seat room ranges from 46 to 61 in (120 to 150 cm) pitch in first, 36 to 39 in (91 to 99 cm) in business, and 32 to 34 in (81 to 86 cm) in economy.[197]

Cabin interior width is approximately 18 feet (550 cm) at armrest,[197] which is 1 inch (2.5 cm) more than originally planned.[198] The Dreamliner's cabin width is 15 inches (38 cm) more than that of the Airbus A330 and A340,[199] 5 inches (13 cm) less than the A350,[200] and 16 in (41 cm) less than the 777.[201] Airlines use economy seat widths that range from 16.33 in (41.5 cm) to 20.66 in (52.5 cm),[202] although published seat research studies recommend a minimum 18-inch (45.7 cm) seat width.[203] 787 economy seats are approximately 17.2 in (43.7 cm) for nine-abreast seating and 19 inches (48 cm) wide for eight-abreast seating arrangements. Most airlines are selecting the nine-abreast (3?3?3) configuration.[204] Boeing engineers designed the 787 interior to better accommodate persons with mobility, sensory, and cognitive disabilities. For example, a 56 in (140 cm) by 57 in (140 cm) convertible lavatory includes a movable center wall that allows two separate lavatories to become one large, wheelchair-accessible facility.[205]

The 787's larger windows are designed to improve passenger views.

The 787's cabin windows are larger in area than all other civil air transports in-service or in development,[206] with dimensions of 10.7 by 18.4 in (27 by 47 cm),[206] and a higher eye level so passengers can maintain a view of the horizon.[207] The composite fuselage permits larger windows without the need for structural reinforcement.[208] Electrochromism-based "auto-dimming" (smart glass) instead of window shades, supplied by PPG Industries,[209] reduce cabin glare while maintaining transparency.[207] The 787's cabin features light-emitting diodes (LEDs)[210] as standard equipment,[211] allowing the aircraft to be entirely 'bulbless'. LED lights have previously been an option on Airbus aircraft and the 777.[211] The system is based on three color LEDs instead of fluorescent tubes,[210] allowing any color and brightness.

The internal cabin pressure of the 787 is increased to the equivalent of 6,000 feet (1,800 m) altitude instead of the 8,000 feet (2,400 m) on older conventional aircraft.[212] According to Boeing, in a joint study with Oklahoma State University, this will significantly improve passenger comfort.[175][213] Cabin air pressurization is provided by electrically driven compressors, rather than traditional engine-bleed air, thereby eliminating the need to cool heated air before it enters the cabin.[214][215] The cabin's humidity is programmable based on the number of passengers carried, and allows 15% humidity settings instead of the 4% found in previous aircraft.[212] The composite fuselage avoids the metal fatigue associated with higher cabin pressure, and eliminates the risk of corrosion from higher humidity levels.[212] The cabin air-conditioning system improves air quality by removing ozone from outside air, and besides standard HEPA filters which remove airborne particles, uses a gaseous filtration system to remove odors, irritants, and gaseous contaminants as well as particulates like viruses, bacteria and allergens.[169][216]

## Variants[edit]

Size comparison of the Boeing 787-8 (black outline) with the Boeing 777-300 (gray), 767-300 (teal), and 737-800 (blue).

Boeing has offered three variants of the 787 from the program launch in 2004. The 787-8 is the first variant produced and is to be followed by the 787-9.

### 787-8[edit]

The 787-8 is the base model of the 787 family, with a length of 186 feet (57 m) and a wingspan of 197 feet (60 m) and a range of 7,650 to 8,200 nautical miles (14,200 to 15,200?km), depending on seating configuration. The 787-8 seats 210 passengers in a three-class configuration.[217] The variant was the first of the 787 line to enter service, entering service in 2011. Boeing is targeting the 787-8 to replace the 767-200ER and 767-300ER, as well as expand into new non-stop markets where larger planes would not be economically viable. Two thirds of 787 orders are for the 787-8.[1]

### 787-9[edit]

The 787-9 will be the first variant of the 787 with a "stretched" or lengthened fuselage, seating 250?290 in three classes with a range of 8,000 to 8,500 nautical miles (14,800 to 15,750?km).[218] This variant differs from the 787-8 in several ways, including structural strengthening, a lengthened fuselage, a higher fuel capacity, a higher maximum take-off weight (MTOW), but with the same wingspan as the 787-8.[219] The targeted entry into service (EIS) date, was originally planned for 2010,[220] but by October 2011 deliveries were scheduled to begin in early 2014.[221] Boeing is targeting the 787-9 to compete with both passenger variants of the Airbus A330 and to replace their own 767-400ER. Like the 787-8, it will also open up new non-stop routes, flying more cargo and fewer passengers more efficiently than the 777-200ER or A340-300/500. The firm configuration was finalized on July 1, 2010.[222]

Artist's impression of the stretched 787-9, designed with greater range and payload capability

When first launched, the 787-9 had the same fuel capacity as the other two variants. The design differences meant higher weight and resulted in a slightly shorter range than the 787-8. After further consultation with airlines, design changes were incorporated to add a forward tank to increase its fuel capacity, so it has a longer range and a higher MTOW than the other two variants.[218] Air New Zealand is the launch customer for the 787-9.[223]

### Other variants[edit]

#### 787-3[edit]

This variant was designed to be a 290-seat (two-class) short-range version of the 787 targeted at high-density flights, with a range of 2,500 to 3,050 nautical miles (4,650 to 5,650?km) when fully loaded. Its design used the same basic fuselage as the 787-8. The wing was derived from the 787-8, with blended winglets replacing raked wingtips. The change decreased the wingspan by roughly 25 feet (7.6 m), allowing the 787-3 to fit into more domestic gates, and in particular in Japan. This model would have been limited in its range by a reduced MTOW of 364,000?lb (165,100?kg).[224][N 1]

An artist's impression of the 787-3, which would have featured a shorter wing with winglets.

The ?3 variant was designed to operate on Boeing 757-300/767-200-sized regional routes from airports with restricted gate spacing.[225] Boeing projected that the future of aviation between very large, but close cities of five million or more people may stabilize around the capacity level of the 787-3.[226][227]

Forty-three 787-3s were ordered by the two Japanese airlines, but production problems on the base 787-8 model led Boeing to postpone the introduction of the 787-3 in April 2008, following the 787-9 but without a firm delivery date.[65] By January 2010, all 787-3 orders had been converted to the 787-8.[228] At the time, it was likely the 787-3 variant would be shelved entirely following the lack of interest by potential customers caused by its being designed specifically for the Japanese market.[229] On December 13, 2010, Boeing canceled the 787-3, since it was no longer financially viable after its orders were canceled.[230]

#### 787-10[edit]

Boeing has stated that it is likely to develop another version, the longer 787-10, with seating capacity between 290 and 310.[231][232] This proposed model is intended to compete with the planned Airbus A350-900.[233] The 787-10 would supersede the 777-200ER in Boeing's current catalog and could also compete against the Airbus A330-300 and A340-300/500. Boeing was having discussions with potential customers about the 787-10 in 2006 and 2007.[234][235][236] In March 2006 Mike Bair, the head of the 787 program at the time, stated that "It's not a matter of if, but when we are going to do it ... The 787-10 will be a stretched version of the 787-9 and sacrifice some range to add extra seat and cargo capacity."[237] Boeing has not yet officially launched the ?10, but it remains under consideration as of 2012.[238][239]

#### Further proposals[edit]

Although no date has been set, Boeing expects to build a 787 freighter version, possibly in 10 to 15 years.[240] Boeing is reported to be also considering a 787 variant as a candidate to replace the 747-based VC-25 as Air Force One.[241]

## Operators[edit]

- All Nippon Airways first service October 26, 2011[155]
- Japan Airlines first service on May 1, 2012[242]
- Ethiopian Airlines first service on August 16, 2012[243]
- Air India first service on September 19, 2012[244]
- LAN Airlines first service on October 1, 2012[245]
- United Airlines first service on November 4, 2012[246][247]
- Qatar Airways first service on November 20, 2012.[248]
- LOT Polish Airlines received its first 787 on November 14, 2012; first service to begin in December 2012.[249]

## Orders and deliveries[edit]

Main article: List of Boeing 787 orders and deliveries

The 787 was first officially delivered to launch customer All Nippon Airways in September 2011.[250] The top three customers for the 787 as of August 2012 are ILFC (International Lease Finance Corporation) with orders totaling 74 Boeing 787s (33 -8s and 41 -9s), All Nippon Airways with 66 orders (36 -8s and 30 -9s) and United Airlines with 50 orders (36 -8s and 14 -9s).[1][251] Qantas also had 50 orders (15 -8s and 35 -9s) but converted the 787-9 orders to options because of the delays and to reduce near term costs.[252]

Net orders and deliveries (cumulative by year)
Data through November 13, 2012[253][1][254]

Boeing 787 total firm orders[1]
787-8 | 787-9 | Unspecified and VIP | Total orders
523 | 315 | 6[253] | 844

Orders and deliveries by year
| 2004 | 2005 | 2006 | 2007 | 2008 | 2009 | 2010 | 2011 | 2012 | Total
Net orders | 56 | 235 | 157 | 369 | 93 | -59 | -4 | 13 | -16[253] | 844
Deliveries | ? | ? | ? | ? | ? | ? | ? | 3 | 30 | 33

- Data through November 13, 2012[253][1][254][255][256]

## Specifications[edit]

Schematic of the Boeing 787-8: side, top, front, cross-section views

Model | 787-8 | 787-9
--- | --- | ---
Cockpit crew | Two
Seating, typical | 242 (3-class) 264 (2-class) | 250?290 280 (3-class)
Length | 186 ft (56.7 m) | 206 ft (62.8 m)
Wingspan | 197 ft 0 in (60.0 m)
Wing area | 3,501 sq ft (325 m2)
Wing sweepback | 32.2 degrees
Height | 55 ft 6 in (16.9 m)
Fuselage dimensions | Width: 18 ft 11 in (5.77 m) / Height: 19 ft 7 in (5.97 m)
Maximum cabin width | 18 ft (5.49 m)
Cargo capacity | 4,822 cu ft (137 m3) 28? LD3 or 9x (88x125) pallets or 8x (96x125) pallets 2x LD3 | 6,086 cu ft (172 m3) 36? LD3 or 11x (88x125) pallets or 11x (96x125) pallets
Maximum takeoff weight | 502,500 lb (228,000 kg) | 553,000 lb (251,000 kg)
Maximum landing weight | 380,000 lb (172,000 kg) | 425,000 lb (193,000 kg)
Maximum Zero-Fuel Weight | 355,000 lb (161,000 kg) | 400,000 lb (181,000 kg)
Operating empty weight | 242,000 lb (110,000 kg) | 254,000 lb (115,000 kg)
Cruising speed | Mach 0.85 (567?mph, 490 knots, 913?km/h at 35,000?ft/10,700?m)[257]
Maximum speed | Mach 0.89 (593?mph, 515 knots, 954?km/h at 35,000?ft/10,700?m)
Range, fully loaded | 7,650–8,200 nmi (14,200–15,200 km; 8,800–9,440 mi) | 8,000–8,500 nmi (14,800–15,700 km; 9,210–9,780 mi)
Take off run at MTOW/SL ISA | 10,300 ft (3,100 m); High Thrust Rating: 8,500 ft (2,600 m)[258] |
Maximum fuel capacity | 33,528 US gal (126,920 L) | 36,641 US gal (138,700 L)
Service ceiling | 43,000 ft (13,100 m)
Engines (?2) | General Electric GEnx or Rolls-Royce Trent 1000
Thrust (?2) | 64,000 lbf (280 kN) | 71,000 lbf (320 kN)

Sources: 787 brochure,[219] 787-8 Airport report,[259] 787 fact sheets[217][218]

## See also[edit]

| Aviation portal

External images
Boeing 787 cutaway
Boeing 787-8 cutaway from Flight International

- Competition between Airbus and Boeing

Related development

- Boeing Sonic Cruiser
- Boeing 747-8
- Boeing Yellowstone Project

Aircraft of comparable role, configuration and era

- Boeing 767
- Airbus A330
- Airbus A350

Related lists

- List of civil aircraft
- List of Boeing 787 orders

## References[edit]

Notes

1. ^ Actual range is based on remaining available weight for fuel after the aircraft empty weight and payload are subtracted from the MTOW.

Citations

1. ^ a b c d e f g Report "787 Model Orders and Deliveries summary". Boeing. October 2012. Retrieved November 17, 2012.
2. ^ Gates, Dominic (September 24, 2011). "Boeing celebrates 787 delivery as program's costs top $32 billion". The Seattle Times. Retrieved September 26, 2011.
3. ^ a b "Boeing Commercial Airplanes prices". Boeing. Retrieved August 7, 2012.
4. ^ a b c d e f g h i j k Norris, G.; Thomas, G.; Wagner, M. and Forbes Smith, C. (2005). Boeing 787 Dreamliner ? Flying Redefined. Aerospace Technical Publications International. ISBN 0-9752341-2-9.
5. ^ "Commercial Airplanes ? 787 Dreamliner ? Background" (Press release). Boeing. Retrieved December 14, 2010.
6. ^ "Flight Standardization Board Report". Federal Aviation Administration. August 25, 2011. Retrieved November 8, 2011.
7. ^ "Boeing Gives the 7E7 Dreamliner a Model Designation" (Press release). Boeing. January 28, 2005. Retrieved June 14, 2011.
8. ^ "Boeing Celebrates the Premiere of the 787 Dreamliner" (Press release). Boeing. July 8, 2007. Retrieved January 21, 2011.
9. ^ Gunter, Lori (July 2002). "The Need for Speed, Boeing's Sonic Cruiser team focuses on the future". Boeing Frontier magazine. Retrieved January 21, 2011.
10. ^ Banks, Howard (May 28, 2001). "Paper plane: That Mach 0.95 Sonic Cruiser from Boeing will never fly. Here's why.". Forbes. Retrieved June 7, 2007.
11. ^ Associated Press. "History of the Boeing 787". Seattle Times, June 23, 2009. Retrieved October 28, 2012.
12. ^ Cannegieter, Roger. "Long Range vs. Ultra High Capacity". Aerlines.nl. Retrieved April 8, 2010.
13. ^ Babej, Marc E.; Pollak, Tim (May 24, 2006). "Boeing Versus Airbus". Forbes. Retrieved April 8, 2010. Text "and Tim Pollak " ignored (help)
14. ^ "Maximizing the Middle, Finding the sweet spot in the market" (Press release). Boeing Frontier magazine. March 2003.
15. ^ "Boeing Achieves 787 Power On" (Press release). Boeing. June 20, 200. Check date values in: `|date=` (help)
16. ^ "Daydream believer: How different is the Boeing 787?". Flight International. Retrieved December 14, 2010.
17. ^ "'Name Your Plane' sweepstakes". Boeing Frontiers Online. July 2003. Retrieved September 28, 2007.
18. ^ Norris & Wagner 2009, p. 40
19. ^ "Boeing Launches 7E7 Dreamliner" (Press release). Boeing. April 26, 2004. Retrieved June 14, 2011.
20. ^ "ANA says Denver still in hunt for non-stop to Tokyo". Metrodenver.org. April 8, 2009. Retrieved December 14, 2010.
21. ^ a b Shifrin, Carole (March 27, 2006). "Dream start". Flight International. Retrieved September 7, 2011.
22. ^ "The Dream of Composites ? RD Magazine". Rdmag.com. November 20, 2006. Retrieved November 23, 2012.
23. ^ Walz, Martha (November 20, 2006). "The Dream of Composites". Rdmag.com (Advantage Business Media). Retrieved September 2, 2011.
24. ^ Norris, Guy (January 9, 2009). Rules Out 787 Window Change "Boeing Rules Out 787 Window Change". Aviation Week. Retrieved June 14, 2011.
25. ^ Ogando, Joseph (June 7, 2007). "Design News ? Features ? Boeing's 'More Electric' 787 Dreamliner Spurs Engine Evolution". designnews.com. Retrieved September 7, 2011.
26. ^ Norris & Wagner 2009, p. 48
27. ^ Pandey, Mohan (2010). How Boeing Defied the Airbus Challenge. USA: Createspace. ISBN 978-1-4505-0113-2.
28. ^ Marsh, George. "Boeing's 787: trials, tribulations, and restoring the dream". Reinforced Plastics. Retrieved July 29, 2010.
29. ^ "Boeing boosts aircraft prices 5.5% on rising cost of labor, materials". Air Transport World. June 26, 2007. Retrieved September 2, 2011.
30. ^ "Boeing Unveils 787 Final Assembly Factory Flow." Boeing, December 6, 2006. Retrieved September 2011 3, 2011.
31. ^ "Boeing's Big Dream", Fortune Magazine, May 5, 2008, p. 182. (online version).
32. ^ "Boeing unveils 787 Dreamliner; Airbus sends congrats". USA Today. July 9, 2007. Retrieved September 2, 2011.
33. ^ Boeing's Big Dream, Fortune, May 5, 2008, p. 187.
34. ^ "Boeing's Big Dream", Fortune, May 5, 2008, p. 184
35. ^ Seo, Sookyung (September 29, 2010). "Boeing 787 Supplier Korea Aerospace Hires Share-Sale Arrangers". Bloomberg. Retrieved September 2, 2011.
36. ^ "Boeing Completes Acquisition of Vought Operations in South Carolina ? Jul 30, 2009" (Press release). Boeing. July 30, 2009. Retrieved September 2, 2011.
37. ^ Gates, D. (September 11, 2005). "Boeing 787: Parts from around world will be swiftly integrated". The Seattle Times. Retrieved September 2, 2011.
38. ^ "Korean Air to Buy 10 ?787 Dreamliners?". KoreaTimes. July 12, 2007.
39. ^ Brochures | Case studies | Whitepapers | Research Papers | Podcasts | Resources- HCL Technologies
40. ^ "India's Tata Group to supply parts for Boeing Dreamliner". AFP. February 6, 2008. Retrieved February 7, 2008.
41. ^ Bhagwat, Ramu (February 7, 2008). "Tatas to make Boeing 787 parts at Mihan". Times News Network. Retrieved September 2, 2011.
42. ^ a b "787 Dreamliner International team facts" (Press release). Boeing. Retrieved June 10, 2010.
43. ^ "Korean Air ready for 787 ramp up". BrisbaneTimes. September 30, 2010. Retrieved September 3, 2011.
44. ^ Boeing's Big Dream, Fortune May 5, 2008, p.189
45. ^ Coulom, Dan (August 20, 2007). "Hamilton Sundstrand delivers first cabin air conditioning packs for Boeing 787 Dreamliner". Press Release. Hamilton Sundstrand. Archived from the original on August 28, 2007. Retrieved August 21, 2007.
46. ^ "Boeing considers moving 787-9 tail build in-house". ATW Online. October 30, 2010. Retrieved October 30, 2010.
47. ^ Gates, Dominic (May 15, 2007). "Boeing shares work, but guards its secrets". Seattle Times. Retrieved September 2, 2011.
48. ^ "International Lease Finance Corp". ATW Online. Penton Media, Inc. November 12, 2007.
49. ^ "Boeing Still Working On 787 Weight Issue, Carson Says". Associated Press. December 7, 2006.
50. ^ "Boeing to deliver test 787s to its customers". Financial Times. July 6, 2007.
51. ^ Wallace, James (December 7, 2006). "Virtual rollout of the 78". Seattle Post-Intelligencer (Hearst Communications Inc). Retrieved September 2, 2011.
52. ^ "Boeing Celebrates the Premiere of the 787 Dreamliner" (Press release). Boeing. July 8, 2007. Retrieved June 14, 2011.
53. ^ Trimble, Stephen (September 10, 2007). "Boeing 787 first flight suffers two-month delay". Flight International. Retrieved September 2, 2011.
54. ^ "Boeing Revises 787 First Flight and Delivery Plans; Adds Schedule Margin to Reduce Risk of Further Delays" (Press release). Boeing. April 9, 2008. Retrieved September 2, 2011.
55. ^ "Final Assembly Begins on Another Boeing 787 Dreamliner" (Press release). Boeing. February 15, 2008. Retrieved September 2, 2011.
56. ^ "Boeing's Big Dream", Fortune Magazine, May 5, 2008, p. 182.
57. ^ "Boeing Delays 787's First Flight to November?December (Update4)". Bloomberg. September 5, 2007. Retrieved September 3, 2011.
58. ^ Carpenter, Dave (October 10, 2007). "Boeing Delays First 787s by Six Months". Yahoo!. Associated Press. Archived from the original on October 12, 2007. Retrieved December 22, 2007.
59. ^ Clark, Nicola (October 10, 2007). "Boeing Delays Deliveries of 787". The New York Times. Retrieved December 22, 2007.
60. ^ "Boeing Reschedules Initial 787 Deliveries and First Flight". Boeing. October 10, 2007. Retrieved September 3, 2011.
61. ^ "787 Program Chief Replaced at Boeing". New York Times. Associated Press. October 17, 2007. Retrieved November 24, 2007.
62. ^ "Boeing Shifts Schedule for 787 First Flight" (Press release). Boeing. January 16, 2008.
63. ^ Buys Vought Share Of Fuselage Builder "Boeing Buys Vought Share Of Fuselage Builder". Aviation Week. March 28, 2008. Retrieved June 14, 2011.
64. ^ Sanders, Peter (July 8, 2009). "Boeing Sets Deal to Buy a Dreamliner Plant". Wall Street Journal.
65. ^ a b "787 variants delayed to at least 2012". Flight International. April 4, 2008.
66. ^ Gates, Dominic (November 5, 2008). "Fasteners incorrectly installed". The Seattle Times. Retrieved November 11, 2008.
67. ^ "New delay". [dead link]
68. ^ "Boeing Reviews Dreamliner Schedule for More Delays (Update2)". Bloomberg. December 4, 2008. Retrieved September 2, 2011.
69. ^ "Boeing confirms 787 first flight pushed back to 2Q 2009". Flight International. December 11, 2008. Retrieved December 14, 2010.
70. ^ "United may seek damages for 787 delays". PSBJ. February 27, 2012. Retrieved March 14, 2012.
71. ^ "Govt approves Air India compensation package for Dreamliner delay". July 25, 2012. Retrieved July 25, 2012.
72. ^ "AI summons Boeing team". Hindustan Times. November 25, 2012.
73. ^ "European and US regulators certify Trent 1000 for Boeing 787". Flight International. Retrieved December 14, 2010.
74. ^ "Boeing performs crash test on 787 fuselage section". KOMO News. August 23, 2007. Retrieved September 28, 2009.
75. ^ a b Snyder, Sean, Associate Editor (August 29, 2007). "Boeing Performs Crash Test on 787 Dreamliner: Tests currently under analysis". Design News. Reed Business Information, a division of Reed Elsevier Inc. Retrieved September 9, 2011.
76. ^ Gillespie, Elizabeth M. (September 6, 2007). "Boeing Says 787 Fuselage Test a Success". Forbes. Retrieved September 7, 2007. [dead link]
77. ^ Snyder, Sean, Associate Editor (September 6, 2007). "Announcement of Boeing Fuselage Crash Test Results". Design News. Reed Business Information. Retrieved September 9, 2011.
78. ^ a b c Gates, Dominic (September 18, 2007). "Fired engineer calls 787's plastic fuselage unsafe". Seattle Times. Retrieved November 24, 2007.
79. ^ a b Matlack, Carol (June 26, 2009). "More Boeing 787 Woes as Qantas Drops Order". Bloomberg BusinessWeek. Retrieved December 14, 2010.
80. ^ "GEnx-1B Engine Receives FAA Certification". Press Release. GE Aviation. March 31, 2008. Retrieved April 4, 2008.
81. ^ "PowerOn Interactive Site". Poweron.tpninteractive.com. Retrieved December 14, 2010.
82. ^ "Boeing Completes 787 Dreamliner 'High Blow' Test" (Press release). Boeing. September 27, 2008. Retrieved September 2, 2011.
83. ^ "FAA Approves Boeing 787 Dreamliner Maintenance Program" (Press release). Boeing. December 22, 2008. Retrieved September 2, 2011.
84. ^ "Boeing 787 Dreamliner Moves to Flight Line for Testing" (Press release). Boeing. May 3, 2009. Retrieved May 3, 2009.
85. ^ "Bernstein Research sees further 787 delays, bigger range shortfall". ATW Daily News, May 4, 2009. Retrieved September 9, 2011.
86. ^ Ostrower, Jon. "Boeing confirms 787 weight issues". Flight International, May 7, 2009. Retrieved September 2, 2011.
87. ^ Ostrower, Jon. "Concerns raised over expected 787 range shortfall". Flight International, March 9, 2009. Retrieved September 2, 2011.
88. ^ Ostrower, Jon. "Shanghai casts doubt over early 787 delivery slots". Flight International, March 14, 2009. Retrieved September 2, 2011.
89. ^ "Boeing Postpones 787 First Flight" (Press release). Boeing. June 23, 2009.
90. ^ Gates, Dominic (July 30, 2009). "Boeing 787 wing flaw extends inside plane". Seattletimes.nwsource.com. Retrieved December 14, 2010.
91. ^ "Dreamliner 787 Composites Approach Takes Another Big Hit". Design News. September 10, 2009. Retrieved September 11, 2009.
92. ^ "Boeing Announces New 787 Schedule and Third-Quarter Charge" (Press release). Boeing. August 27, 2009.
93. ^ Gates, Dominic (August 28, 2009). "Boeing still sure delayed 787 will be profitable". The Seattle Times. Retrieved September 23, 2009.
94. ^ a b Cohen, Aubrey. "Boeing illegally put second 787 line in S.C., complaint says." Seattlepi.com, April 20, 2011. Retrieved September 2, 2011.
95. ^ Ostrower, Jon (December 13, 2009). "Boeing clears 787 to fly 15 December". Air Transport Intelligence. Retrieved September 2, 2011.
96. ^ "Boeing Completes 787 Dreamliner High-Speed Taxi Test" (Press release). Boeing. December 12, 2009. Retrieved September 3, 2011.
97. ^ "787 approaches final gauntlet testing". Flight International. December 8, 2009. Retrieved December 15, 2009.
98. ^ Ostrower, Jon (December 15, 2009). "Boeing 787 Dreamliner lifts off on maiden flight". Flight International. Retrieved September 2, 2011.
99. ^ "Boeing 787 jet lands after maiden flight". Ninemsn.com.au, December 16, 2009. Retrieved September 9, 2011.
100. ^ Ostrower, Jon (December 15, 2009). "Boeing completes 787 maiden sortie". Flightglobal. Retrieved December 16, 2009.
101. ^ "Boeing Dreamliner completes first flight". BBC News. December 15, 2009. Retrieved September 9, 2011.
102. ^ Mecham, Michael and Guy Norris. Plans 8.5 Months Of 787 Testing "Boeing Plans 8.5 Months Of 787 Testing". Aviation Week, December 18, 2009. Retrieved June 14, 2011.
103. ^ "The B777". Triple7 World site
104. ^ Boeing Commercial Airplane Group No.2 > December 22, 2009 > KPAE-KBFI. FlightAware.com
105. ^ "Second Boeing 787 Dreamliner Completes First Flight". Boeing, December 22, 2009. Retrieved September 2011.
106. ^ a b "787 Dreamliner Flight Test site". Boeing. Retrieved August 15, 2011.
107. ^ Ostrower, Jon. "Boeing completes 787 flutter and ground effects testing". Flight International, March 24, 2010. Retrieved September 3, 2011.
108. ^ "Boeing Completes Ultimate-Load Wing Test on 787" (Press release). Boeing. March 28, 2010. Retrieved March 30, 2010.
109. ^ Sanders, Peter (March 30, 2010). and Aerospace_leftHeadlines/ "Boeing's Dreamliner Lags Testing Schedule". Wall Street Journal. Retrieved September 2, 2011.
110. ^ Paur, Jason (March 29, 2010). "Boeing 787 Passes Incredible Wing Flex Test". Wired.
111. ^ "Boeing Confirms Success on 787 Wing, Fuselage Ultimate Load Test" (Press release). Boeing. April 7, 2010.
112. ^ "Boeing 787 in hot/cold testing in Florida". UPI.com, April 23, 2010. Retrieved September 3, 2011.
113. ^ "First 787 GEnx Engine Runs Complete". Boeing, May 12, 2010.
114. ^ "VIDEO: GEnx powered 787 completes maiden flight". Flight International. Retrieved July 21, 2010.
115. ^ "Horizontal stabiliser gaps force 787 inspections and reduced flight envelope". flightglobal. June 25, 2010. Retrieved June 26, 2010.
116. ^ a b Jason Paur (June 17, 2010). "Boeing 787 Withstands Lightning Strike". Wired.
117. ^ "FAA Probes American's Inspections". Wall Street Journal, May 16, 2008, p. B1
118. ^ Gates, Dominic. "Building the 787, When lightning strikes". Seattle Times, March 5, 2006. Retrieved September 3, 2011.
119. ^ Gates, Dominic (February 8, 2009). "FAA to loosen fuel-tank safety rules, benefiting Boeing's 787". The Seattle Times. Retrieved September 2, 2011.
120. ^ "Dreamliner lands at Farnborough". BBC News, July 18, 2010. Retrieved July 18, 2010.
121. ^ Mustoe, Howard (August 24, 2010). "Rolls-Royce Blowout Shutters Boeing, Airbus Test Bed". Bloomberg. Retrieved August 29, 2010.
122. ^ "Boeing delays delivery of 787 aircraft until next year". BBC. August 27, 2010. Retrieved August 27, 2010.
123. ^ Ostrower, Jon (August 28, 2010). "Lack of production engine for Airplane Nine drives 787 delay". Flight International. Retrieved August 29, 2010.
124. ^ "Boeing faces claim on 787 delays; sixth flight test aircraft won't fly until September". ATW Online. August 16, 2010. Retrieved August 16, 2010.
125. ^ "787 flight test fleet to expand". ATW Online. September 10, 2010. Retrieved September 9, 2010.
126. ^ Norris, Guy. 787 Suffers Engine Surge During Tests "Boeing 787 Suffers Engine Surge During Tests". Aviation Week, September 16, 2010. Retrieved June 14, 2011.
127. ^ "Sixth Boeing 787 Makes First Flight, Testing Program Making Good Progress". Boeing, October 4, 2010.
128. ^ "Boeing faces prospect of further 787 delay". Flight International. November 5, 2010. Retrieved November 6, 2010.
129. ^ "JAL hit by further 787 delivery delay". Air Transport Intelligence. November 4, 2010. Retrieved November 6, 2010.
130. ^ Koenig, David (November 9, 2010). "Boeing 787 makes emergency landing on test flight". Associated Press. Retrieved September 9, 2011.
131. ^ Gates, Dominic (November 9, 2010). "Electrical fire forces emergency landing of 787 test plane". The Seattle Times. Retrieved November 9, 2010.
132. ^ "Boeing 787 Makes Emergency Landing On Test Flight". National Public Radio. Associated Press. November 9, 2010. Retrieved November 9, 2010. [dead link]
133. ^ "787 electrical fire raises prospect of further delay". Retrieved November 15, 2010.
134. ^ Norris, Guy. "787s Grounded After Emergency Landing". Aviation Week, November 10, 2010. Retrieved June 14, 2011.
135. ^ Norris, Guy. Remain Grounded "787s Remain Grounded". Aviation Week, November 11, 2010. Retrieved June 14, 2011.
136. ^ Rothman, Andrea. "Boeing 787 Fire Sparked by Stray Tool". Bloomberg, November 25, 2010.
137. ^ Ostrower, Jon. "787 flight tests resume, final schedule unclear". Air Transport Intelligence, December 23, 2010. Retrieved September 2, 2011.
138. ^ "Boeing Resumes 787 Flight Testing". Boeing, December 23, 2010.
139. ^ "Boeing Sets 787 First Delivery for Third Quarter" (Press release). Boeing. January 18, 2011. Retrieved September 2, 2011.
140. ^ "Boeing expects first 787 delivery in the third quarter". Flight International. January 18, 2011.
141. ^ Ostrower, Jon (February 24, 2011). "Boeing passes 1,000 787 flights". Air Transport Intelligence. Retrieved September 2, 2011.
142. ^ Koh, Quintella (July 4, 2011). "All Nippon Airways starts week-long 787 validation". Air Transport Intelligence. Retrieved July 6, 2011.
143. ^ Ostrower, Jon. "Certification flight testing complete, the 787 fleet is still busy". Flightblogger on Flightglobal.com, August 15, 2011.
144. ^ Ostrower, Jon. "Boeing confirms 787 certification flight test completion". Air Transport Intelligence, August 17, 2011. Retrieved September 2, 2011.
145. ^ "787 wins certification from FAA and EASA". Air Transport Intelligence. August 26, 2011. Retrieved August 26, 2011.
146. ^ a b c "Press Release ? FAA Approves Production of Boeing 787 Dreamliner". FAA. August 26, 2011. Retrieved August 29, 2011.
147. ^ "Boeing 787 Dreamliner makes first-ever biofuel-powered Pacific crossing" GizMag, 17 April 2012. Retrieved 20 April 2012.
148. ^ Hananel, Sam. "Labor board drops high-profile Boeing complaint" ap.org, December 9, 2011. Retrieved December 12, 2011.
149. ^ Peterson, Kyle (April 27, 2012). "Boeing Debuts First 787 Dreamliner in South Carolina". Reuters. Retrieved 3 May 2012.
150. ^ Ostrower, Jon (September 25, 2011). "Boeing formally delivers first 787 to ANA". Flight International. Retrieved September 26, 2011.
151. ^ Gunter, Lori and Scott Lefeber (September 25, 2011). "Boeing, ANA Complete Contractual Delivery of First 787 Dreamliner". Boeing. Retrieved September 26, 2011.
152. ^ "First delivered Boeing 787 takes off for Japan". Reuters. September 27, 2011. Retrieved September 27, 2011.
153. ^ Associated Press. "All Nippon Airways of Japan takes delivery of first Boeing 787 at Everett, Wash., factory". Washingtonpost.com, September 26, 2011.
154. ^ "Boeing delivers its second 787 and jumbo freighter". The Seattle Times, October 13, 2011.
155. ^ a b c Tim Kelly (October 26, 2011). "Dreamliner carries its first passengers and Boeing's hopes". Reuters. Retrieved October 28, 2011.
156. ^ "Boeing's Dreamliner completes first commercial flight". BBC News. October 26, 2011. Retrieved October 26, 2011.
157. ^ ANA 787 connection website
158. ^ "Boeing 787 Dreamliner Sets Speed, Distance Records". Boeing Press Release, December 8, 2011]
159. ^ "Boeing Announces 787 Dream Tour". Boeing. December 4, 2011. Retrieved February 24, 2012.
160. ^ "Boeing announces next segment of 787 dream tour". Boeing. February 22, 2012. Retrieved February 24, 2012.
161. ^ "787 Dremaliner Dream Tour page". Boeing. Retrieved February 24, 2012.
162. ^ Schofield, Adrian (June 12, 2012). "ANA Says 787s Exceeding Fuel Efficiency Target (subscription article)". Aviation Week. Retrieved June 13, 2012.
163. ^ Creedy, Steve (June 12, 2012). "Rave reviews for Boeing's 787". The Australian (Business with The Wall Street Journal). Retrieved 06/12/2012. Check date values in: `|accessdate=` (help)
164. ^ "FARNBOROUGH: Qatar unveils first 787 at show". Flight International. July 10, 2012. Retrieved July 11, 2012.
165. ^ "NTSB urges grounding for certain GEnx-powered 787 and 747-8s". Flightglobal.com. 2012-09-15. Retrieved 2012-10-01.
166. ^ "AI summons Boeing team". Hindustan Times. November 25, 2012.
167. ^ "Boeing 787: A Matter of Materials ? Special Report: Anatomy of a Supply Chain". IndustryWeek.com, December 1, 2007.
168. ^ "787 Dreamliner Program Fact Sheet". Boeing web page. The Boeing Company. Retrieved July 10, 2007.
169. ^ a b c d e Hawk, Jeff (Director Certification, Government and Environment 787 Programs) (May 25, 2005). "The Boeing 787 Dreamliner: More Than an Airplane" (PDF). Presentation to AIAA/AAAF Aircraft Noise and Emissions Reduction Symposium. American Institute of Aeronautics and Astronautics and Association A?ronautique et Astronautique de France. Retrieved July 15, 2007.
170. ^ a b Zaman, K.B.M.Q.; Bridges, J.E.; Huff, D.L. "Evolution from 'Tabs' to 'Chevron Technology? ? a Review" (PDF). Proceedings of the 13th Asian Congress of Fluid Mechanics 17?21 December 2010, Dhaka, Bangladesh (NASA Glenn Research Center. Cleveland, OH, USA.): pp. 47?63. 1.34 Mb
171. ^ "Boeing 787 program background". Retrieved May 4, 2007.
172. ^ "Boeing 787 from the Ground Up". Boeing, AERO magazine, QTR_04/06
173. ^ "787 No Bleed Systems". Boeing AERO magazine, Quarter 4, 2007.
174. ^ 787 integrates new composite wing deicing system. Composites World, December 30, 2008.
175. ^ a b Croft, John (July 2006). "Airbus and Boeing spar for middleweight" (PDF). Aerospace America (American Institute of Aeronautics and Astronautics). Retrieved July 8, 2007.
176. ^ Universal-type gust alleviation system for aircraft, United States Patent 4905934. freepatentsonline.com, original publication March 6, 1990. Accessed: December 9, 2009.
177. ^ "What is ARINC 661?" Web archive of Engenuity Technologies page.
178. ^ "Boeing Unveils 787 Dreamliner Flight Deck." Boeing, August 31, 2005. Retrieved September 2, 2011.
179. ^ Coppinger, Rob (October 6, 2006). "NASA Orion crew vehicle will use voice controls in Boeing 787-style Honeywell smart cockpit". Flight International. Retrieved October 6, 2006.
180. ^ McHale, John (April 2005). "AFDX technology to improve communications on Boeing 787". Military Aerospace Electronics Magazine (PennWell). Retrieved July 8, 2007.
181. ^ a b c Zetter, Kim (January 4, 2008). "FAA: Boeing's New 787 May Be Vulnerable to Hacker Attack". Wired. Retrieved January 6, 2008.
182. ^ "Special Conditions: Boeing Model 787-8 Airplane; Systems and Data Networks Security?Isolation or Protection From unauthorized Passenger Domain Systems Access". Federal Aviation Administration. U.S Government Printing Office (GPO). January 3, 2008. Retrieved November 1, 2012. "For these design features, the applicable airworthiness regulations do not contain adequate or appropriate safety standards for protection and security of airplane systems and data networks against unauthorized access."
183. ^ "Market Research Report: Strategic Business Expansion of Carbon Fiber, Torayca" (PDF). Toray Industries press release. Toray Industries. April 12, 2005. Archived from the original on February 4, 2007. Retrieved July 9, 2007.
184. ^ "Boeing Testing Sample Sonic Cruiser Fuselage". Boeing. July 24, 2002.
185. ^ "Development Work on Boeing 787 Noses Ahead". Boeing. July 13, 2005. Retrieved June 14, 2011.
186. ^ "Low-Cost Composite Materials and Structures for Aircraft Applications". NATO Research Technology Organisation. May 7?11, 2001. Retrieved July 21, 2010. Check date values in: `|date=` (help)
187. ^ Pike, John (January 4, 2011). "C-17 Globemaster III". Globalsecurity.org. Retrieved January 11, 2011.
188. ^ "Dan Rather Reports ? Boeing 787 composite concerns (1 of 4)". YouTube. November 7, 2007. Retrieved December 15, 2009.
189. ^ Holmes, Stanley (June 19, 2006). "The 787 Encounters Turbulence". BusinessWeek. Bloomberg L.P.
190. ^ "Does composite use in airplane manufacturing trade passenger safety for profits?". Star-Telegram. December 3, 2009. [dead link]
191. ^ Wallace, James (January 9, 2006). "Airbus to use composites". Seattle Post-Intelligencer (Hearst Communications Inc.). Retrieved September 2, 2011.
192. ^ Bickers, Chaz (July 2006). "Good as GoldCare: Revolutionary 787 fleet support program complements airplane's technical achievements" (PDF). Boeing Frontiers (Boeing). Retrieved September 2, 2011.
193. ^ Johnsson, Julie (September 2, 2007). "Boeing coining plan for composite parts". Chicago Tribune (Tribune Interactive, Inc).
194. ^ "GR Boeing Demo. Quiet Technology". Goodrich press release. Goodrich Corporation. August 16, 2005. Archived from the original on October 19, 2007. Retrieved July 10, 2007.
195. ^ Corliss, Bryan (June 21, 2009). "What's new, different about the 787". The Daily Herald. Retrieved January 22, 2011.
196. ^ a b "787 Is not Meeting 24hour-Engine Change Promo, lessor says." Leeham Co. LLC. July 18, 2005.
197. ^ a b "D6-58331, Boeing 787 Airplane Characteristics for Airport Planning" (PDF). Boeing Commercial Aircraft. July 2012. pp. Section 2.4 Interior Arrangements (p. 10); Section 2.5 Cabin Cross?Sections (p. 13).
198. ^ Wallace, James (November 18, 2005). "Boeing details 787 improvements". Seattle Post-Intelligencer (Hearst Communications Inc). Retrieved September 2, 2011.
199. ^ "Airbus A330 and A340 family specifications".
200. ^ "Airbus ? A350 XWB Xtra comfort". Archived from the original on February 5, 2008.
201. ^ "Airbus unveils widebody, says A350 XWB will top 787 and 777". Seattlepi.com. July 18, 2006. Retrieved December 14, 2010.
202. ^ Verghese, Vijay. "A survey of the best airline economy seats". Smarttravelasia.com. Retrieved February 12, 2012.
203. ^ "Anthropometry and Ergonomics in Airline Seating". ?. ?. Check date values in: `|date=` (help)
204. ^ Wallace, James. "Aerospace Notebook: More seats sought on 787". Seattle-PI, February 22, 2006. Retrieved: February 12, 2012.
205. ^ Cram, Jennifer (March 26, 2007). "Boeing Unveils Improved Access Features on the 787". Boeing press release. The Boeing Company. Archived from the original on October 11, 2007. Retrieved July 10, 2007.
206. ^ a b Wallace, James (June 5, 2007). "Aerospace Notebook: In Airbus, Boeing duel, jet windows a shut case". Seattle Post-Intelligencer. Retrieved September 2, 2011.
207. ^ a b Wallace, James (November 26, 2008). "Continental plans Dreamliner seats to be roomy, with a view". Seattle Post-Intelligencer (Hearst Communications Inc). Retrieved November 28, 2008. [dead link]
208. ^ Norris & Wagner 2009, p. 49
209. ^ Norris, Guy (December 20, 2005). "Qantas deal sees launch of 787-9". Flight International. Reed Elsevier.
210. ^ a b "Cabin Interior, Mood Lighting". Diehl Aerospace, Germany. Archived from the original on September 27, 2007. Retrieved May 1, 2007.
211. ^ a b "Diehl Aerospace GmbH: Mood Lighting System". Diehl Aerospace. 2012. Retrieved January 1, 2012.
212. ^ a b c Adams, Marilyn (November 1, 2006). "Breathe easy, Boeing says". USA Today.
213. ^ "Boeing 7E7 Offers Preferred Cabin Environment, Study Finds." Boeing, July 19, 2004. Retrieved June 14, 2011.
214. ^ Ogando, Joseph, Senior Editor (June 4, 2007). "Boeing's 'More Electric' 787 Dreamliner Spurs Engine Evolution: On the 787, Boeing eliminated bleed air and relied heavily on electric starter generators". Design News. Retrieved September 9, 2011.
215. ^ Dornheim, Michael (March 27, 2005). 787 Electrical System Pressurizes Cabin "Massive 787 Electrical System Pressurizes Cabin". Aviation Week Space Technology. Retrieved January 1, 2012.
216. ^ Turner, Edgar (2010). The Birth of the 787 Dreamliner. Kansas City, Missouri: Andrews McMeel Publishing. p. 220. ISBN 978-0-7407-9667-8.
217. ^ a b "Boeing 787-8 Dreamliner Fact Sheet". Boeing. Retrieved November 23, 2007.
218. ^ a b c "Boeing 787-9 Dreamliner Fact Sheet". Boeing. Retrieved November 23, 2007.
219. ^ a b Boeing 787 Airport Compatibility Brochure. Boeing, December 2009.
220. ^ Wallace, J."Aerospace Notebook: New 787 is taking off"[dead link]. Seattle Post-Intelligencer, April 27, 2005.
221. ^ Boeing delays first 747-8I and 787-9 deliveries
222. ^ "Boeing clears firm configuration hurdle for 787-9". flightglobal. 2010. Retrieved July 2, 2010.
223. ^ Norris & Wagner 2009, p. 50
224. ^ "Boeing 787-3 Dreamliner Fact Sheet". Boeing. Archived from the original on November 19, 2007. Retrieved November 23, 2007.
225. ^ Norris & Wagner 2009, p. 38
226. ^ Baseler, Randy (May 20, 2005). "Kangaroo hop". Randy's Journal. The Boeing Company. Retrieved July 10, 2007.
227. ^ Pate, R. Hewitt (Assistant Attorney General, Antitrust Division); McDonald, Bruce (Deputy Assistant Attorney General, Antitrust Division) and Gillespie, William H. (Economist) (May 24, 2005). "Congestion And Delay Reduction At Chicago O'Hare International Airport: Docket No. FAA-2005-20704". Comments of The United States Department of Justice. Before The Federal Aviation Administration Department of Transportation. Retrieved September 2, 2011.
228. ^ Ostrower, Jon (January 8, 2010). "ANA abandons 787-3". Flight International.
229. ^ "Boeing will likely scrap 787-3". The Seattle Times. February 2, 2010. Retrieved February 7, 2010.
230. ^ Ray, Susanna (December 13, 2010). "Boeing raises aircraft prices 5.2%, cancels short-haul 787". Seattle Times.
231. ^ Wallace, James (December 22, 2005). "Everett work force for 787 pegged at 1,000". Seattle Post-Intelligencer. Retrieved September 2, 2011.
232. ^ Thomas, G. (September 26, 2005). "Boeing looks at larger Dreamliner to meet Emirates, BA requirements". Air Transport World. Retrieved September 3, 2011.
233. ^ Thomas, G. (December 23, 2005). "Boeing bullish on 787-10, Dreamliner production". Air Transport World (ATW Media Group). Retrieved September 2, 2011.
234. ^ Baseler, Randy (February 8, 2006). "Dash 10". Boeing Blog. Retrieved November 17, 2011.
235. ^ Cameron, Doug and Kevin Done (July 8, 2007). "Customers guard Boeing 787 delivery slots". Financial Times. Retrieved July 8, 2007.
236. ^ Leach, Yvonne and Gunter, Lori (June 19, 2007). "Boeing Highlights Progress on First 787, Subsequent Airplanes". Boeing Press Release. Retrieved June 23, 2007.
237. ^ "Lunsford, J. Lynn (March 27, 2006). "Boeing to Build Stretch 787 Jet". The Wall Street Journal.
238. ^ Wall, Robert (June 20, 2008). Reconsiders Plan for 787-10channel=awst "Boeing Reconsiders Plan for 787-10". Aviation Week Space Technology. Retrieved June 14, 2011.
239. ^ Thomas, Geoffrey (June 2, 2011). "Bernstein: Boeing moving closer to a 787-10". ATW online. Retrieved November 17, 2011.
240. ^ Ng, J. Boeing executive says no freighter version of 787 is likely for 10 years, Marketwatch from Dow Jones. Retrieved January 2, 2008.
241. ^ Butler, Amy. "Boeing Only Contender for New Air Force One". AviationWeek.com. Retrieved June 14, 2011.
242. ^ "Japan Airlines announces delivery of 787". Japan Airlines. March 21, 2012. Retrieved June 12, 2012.
243. ^ "Ethiopian receives first 787". Flightglobal.com. 2012-08-14. Retrieved 2012-10-01. Text "FGFG" ignored (help); Text "twitterfeed" ignored (help); Text "Flightglobal " ignored (help)
244. ^ "Air India receives third Boeing 787 Dreamliner". Ibnlive.com. 2012-08-14. Retrieved 2012-10-01.
245. ^ {cite web |url=http://finance.yahoo.com/news/boeing-celebrates-delivery-lan-airlines-194100092.html;_ylt=A2KJ3CWVu0ZQ8BAAD8DQtDMD |title=Boeing Celebrates Delivery of LAN Airlines' first 787 Dreamliner |publisher=hub.united.com |date=2012-08-31 |accessdate=2012-10-27}}
246. ^ "United Airlines plans first 787 Dreamliner flight Sunday". Denver Business Journal, November 2, 2012.
247. ^ "United Completes FAA Certification Program for Boeing 787 Operations". airlinesanddestinations.com, November 2, 2012.
248. ^ "Qatar Airways first Boeing 787 takes off to Dubai". India Infoline News. 21 November 2012. Retrieved 28 November 2012.
249. ^ "LOT Polish Airlines takes delivery of its first Boeing 787, becomes the first European carrier to fly the Dreamliner". worldairlinenews.com, November 15, 2012.
250. ^ Michael (August 26, 2011). "Boeing 787 Dreamliner ? Date for First Delivery". Flight Story. Retrieved August 26, 2011.
251. ^ "Boeing resumes 787 production". Flight International. January 30, 2009. Retrieved September 2, 2011.
252. ^ Schofield, Adrian (August 23, 2012). "Qantas may take 787-9s in 2016 despite cancellations". Aviation Week. The McGraw Hill Companies. Retrieved November 17, 2012.
253. ^ a b c d Current orders. Boeing, November 13, 2012. Retrieved: November 19, 2012.
254. ^ a b Annual Orders Summary. Boeing, October 2012. Retrieved: November 19, 2012.
255. ^ "Current Deliveries". Boeing. October 2012. Retrieved November 8, 2012.
256. ^ "Orders and Deliveries search page". Boeing. October 2012. Retrieved November 17, 2012.
257. ^ For same speed of Mach 0.85 at 35,000 ft, Boeing lists 567 mph and 913?km/h on the 747-400's technical characteristics page
258. ^ "D6-58331, Boeing 787 Airplane Characteristics for Airport Planning" (PDF). Boeing Commercial Aircraft. July 2012. p. 25. Retrieved October 10, 2012.
259. ^ "D6-58331, Boeing 787 Airplane Characteristics for Airport Planning" (PDF). Boeing Commercial Aircraft. July 2012. Retrieved October 10, 2012.

Bibliography

- Norris, Guy and Mark Wagner. Boeing 787 Dreamliner. US: Zenith Press, 2009. ISBN 978-0-7603-2815-6.

## External links[edit]

| Wikimedia Commons has media related to: Boeing 787 (category)

- Boeing 787 Dreamliner Official page on newairplane.com
- Boeing 787 page on Boeing.com
- Boeing 787 News on Flightglobal.com
- Boeing 787 Dreamliner on Aerospace-Technology.com
- "Go inside the first 787 Dreamliner" Boeing video tour of ZA001.
- Planemakers confront green issues, by Jorn Madslien, BBC News
- "Boeing 787 Dreamliner completes its maiden flight", BBC news with video

Boeing airliners
Piston-engined | 40A 80 221 247 307 314 377
Jet-engined | 367-80 707/720 717 727 737 737 Classic 737 NG 747 747SP 747-400 747-8 757 767 777 787
In development | 737 MAX 777X
Proposed | Y1 Y3
Not developed | 2707 7J7 New Large Airplane Sonic Cruiser

Boeing 7x7 aircraft production timeline, 1955–present
1950s | 1960s | 1970s | 1980s | 1990s | 2000s | 2010s
5 | 6 | 7 | 8 | 9 | 0 | 1 | 2 | 3 | 4 | 5 | 6 | 7 | 8 | 9 | 0 | 1 | 2 | 3 | 4 | 5 | 6 | 7 | 8 | 9 | 0 | 1 | 2 | 3 | 4 | 5 | 6 | 7 | 8 | 9 | 0 | 1 | 2 | 3 | 4 | 5 | 6 | 7 | 8 | 9 | 0 | 1 | 2 | 3 | 4 | 5 | 6 | 7 | 8 | 9 | 0 | 1 | 2 | 3
| Boeing 707 |  |  |  |
|  |  |  |  | Boeing 717 (MD-95) |  |
|  | Boeing 727 |  |  |  |
|  | Boeing 737
|  | Boeing 747
|  |  |  | Boeing 757 |  |
|  |  |  | Boeing 767
|  |  |  |  | Boeing 777
|  |  |  |  |  | Boeing 787
= Narrow-body | = Wide-body

Boeing model numbers
Aircraft | 1 2 3 4 5 6 6D 6E 7 8 10 15 16 21 40 42 50 53 54 55 58 63 64 66 67 68 69 72 74 75 77 80 81 83 89 93 95 96 99 100 101 102 200 202 203 204 205 214 215 218 221 222 223 226 227 234 235 236 246 247 248 251 256 264 266 267 273 280 281 294 299 300 306 307 314 316 344 345 367 367-80 377 400 450 451 464 466 474 479 701 953 707 717 (i) 717 (ii) 720 727 733 737 739 747 757 767 777 787 2707
Turbine engines | 502 520 550
Vessels | 929
Other | Boeing Customer Codes

Lists relating to aviation
General | Aircraft manufacturers Aircraft engines manufacturers Gliders Airlines defunct Airports Civil authorities Museums Registration prefixes Rotorcraft manufacturers Timeline
Military | Air forces Weapons Experimental Missiles Unmanned
Accidents/incidents | Commercial airliners by location Fatalities by death toll General aviation Military
Records | Airspeed Altitude Distance Endurance Firsts Large Most-produced aircraft Most-produced rotorcraft