['Product details\nSATAjet 5000 B\nFlexible. Ergonomic. Easy handling.\nWith the SATAjet 5000 B, painters can adjust the inlet pressure and the painting distance according to the paint used, the climatic conditions and their working style – and achieve perfect results in any situation. The ergonomic paint spray gun has been developed in cooperation with the Porsche Design Studio – to ensure perfect ergonomics. Robust and light – with ergonomic adjustment elements, the SATAjet 5000 B ensures comfortable working.\nFor 360° view\nProduct Benefits\nFlexible application: Optimized nozzle concept for various spray distances and inlet pressures\nErgonomic design: Pleasant and compact handle shape combined with easy-to-operate control elements\nEasy cleaning: PerloxalTM surface for improved corrosive properties and even easier cleaning and maintenance\nFast assembly: The paint needle can be mounted easily, safely and quickly thanks to the positionally secure clip roller\nFine adjustment: Optimised round /', 'DIY homeowners, including those new to paint sprayers, breeze through paint jobs with the Magnum Project Painter Plus. This sprayer has the capacity to handle most interior and exterior home improvement projects and lets you spray directly from a 1 or 5 gallon container to finish faster.', "Whether you're looking for a quality paint sprayer, are an avid Do-It-Yourselfer, or simply want to paint the easy and fun way, the Finish Max is for you! The Finish Max sprays a smooth, factory-like finish with no compressor required. \n The Finish Max paint sprayer lays down a fine, quality finish with minimal overspray. Applies paint or stain quickly, saving time when compared to using a brush or roller. Ideal for spraying crafts, dressers, doors, furniture and cabinets.        \n\nFeatures\n\nIdeal for small to medium projects (furniture, crafts, dressers, cabinets, etc.)\n\nSpray chalk-type paints, cabinet paints, furniture paints, stain, poly and latex\n\n2.0 mm brass spray tip and durable housing for longer life and improved performance\n\nThree different spray patterns: horizontal, vertical, and circular\n\nAdjust the trigger control knob to change spray pattern from 1” to 6” wide\n\n400 watts of power\n\n27 ounce container capacity\n\nSprays evenly to lay down a professional finish", 'The Paasche TG is a double action gravity feed airbrush. The airbrush features a chrome plated body and anodized aluminum handle for durability. The TG is our finest detail airbrush allowing the user to achieve hair line detail and using the included fan head wider patterns up to 3 inches. A PTFE packing allows the TG to handle any water or solvent based paint. Clean up is as simple as spraying your paint cleaner though the airbrush and wiping of the needle. The TG is best used for those requiring high end detail. Applications including automotive graphics, models, taxidermy, cake decorating, tattoos, finger nails, graphic arts, illustration, etc. The TG airbrush is made and assembled in the USA.\nTG-3WC Includes:\nTG#2 Double Action Airbrush, wood case, .4 oz cup, cup cover, size 1 and 3 heads, fan aircap, Hanger, 2 wrenches, 6ft braided hose, lessons booklet and manual.\nFeatures:\nAirbrush Made In The USA\nQuality precision materials for fine detail work\nHighly polished & hardened stainl', 'What is the difference between the Fuji Spray® Mini-Mite PLATINUM™ and Q PLATINUM™ turbine?\n\nToday we are going to answer this age-old question:\n\nThe main difference between the Mini-Mite PLATINUM™ and Q PLATINUM™ turbines is – \nnoise level\n. The Q PLATINUM™ series is designed with patented noise reduction technology that reduces the sound of the motor by eliminating all Direct Sound Paths found commonly on low to mid-priced HVLP turbines. While a comparable sound level to the Mini-Mite PLATINUM™ turbine is a standard shop vacuum system – the Q PLATINUM™ series will reduce those levels by 50%.\n\nFor example, at 20ft away, the Q5 PLATINUM™ runs at 60dba, which would be similar to a normal conversation:\n\nAt 15ft, the Q4 PLATINUM™ Turbine is only 62 dba, and at 20ft it is 59 dba.\n\nAt 15ft, the Q3 PLATINUM™ Turbine is only 61 dba, and at 20ft, it is 58 dba.\n\nWhich series is best for you?\n\nThe Q PLATINUM™ series\n is an ideal turbine system for use where sound levels \nare\n a factor. Especiall', 'Great for painting or staining large projects\nHigh Efficiency Airless technology reduced up to 55% less overspray\nPour 1.5 gal. of paint right into the hopper\n\nFeatures\n\nGravity fed for fast, no mess priming and cleaning\nHolds up to 1.5 gallons of material right in the tank for continuous painting\nCovers 8′ x 10′ wall in 2 minutes\n515 HEA Spray Tip puts out a 10 inch spray pattern and is great for latex paints\n25 foot hose for easy, two-story reach\nLong hose allows movement flexibility and great for when working on a ladder\nSpill resistant lid keeps debris out of paint and is easy to move around projects\nEquipped with integrated handles and tip storage\nSimply rinse and flush the system for quick cleanup\n\nDetails\n\nThe new Control Pro 130 Power Tank is ideal for big interior and exterior jobs and can be used with a wide range of unthinned paints and stains. It takes the intimidation out of airless spraying with fast and easy set up and unmatched control, all while delivering continuous p', 'The FX3000 is a full size HVLP spray gun for larger jobs and the gun of choice when HVLP is required.\n\nInnovations of the Finex gun include 29% fewer parts, precision lids, repair kits, optional 3M\n™\n\n\tPPS\n™\n adapter, optional interchangeable aluminum cups and lowest trigger pull among all guns in its class.\n\nFeatures\n\nTechnical Specs\n\nApplications\n\nDownloads\n\nLarge pattern size, up to 12.5 inches \n\nHVLP gun with multiple nozzles ranging from 1.0 to 1.8 spray primer, base, and clear\n\nIncludes FX3000 gun, 600cc aluminum cup, wrench and cleaning brush \n\nOne year warranty\n\nFluid Tips:\n 1.0 mm, 1.3 mm, 1.4 mm, 1.5 mm, 1.8 mm\n\nAir Consumption (cfm):\n 9.5 SCFM\n\nMax Inlet HVLP psi:\n 29 psi (2.0 bar, 200 kPa)\n\nWeight With  Cup:\n 1.11 lb \n\nAir Inlet npsm:\n 1/4 in\n\nFinish:\n Black Nickel\n\nCup Size:\n 600 cc\n\nPattern Size:\n 12.5 in\n\nWarranty:\n 1 year\n\nTip Size (mm)\n\nGun Part Number\n\nNeedle, Nozzle, Air Cap Kit Part Number\n\n1.0\n\n288878\n\n289296\n\n1.3\n\n288879\n\n289297\n\n1.4\n\n288880\n\n289298\n\n1.5\n\n288881\n\n']