['The\xa0\nLeica DISTO D1\n\xa0is the first in line of the\nDISTO Family\n of \nBluetooth Laser Distance Meters\n. This simple model has been stripped back to just the basics. The\xa0\nDISTO D1\n gives easy, quick and accurate interior measurements. It is perfectly small, light and fits easily into a pocket or handbag. Whether you are measuring for flooring, curtains or hanging pictures on a wall, the \nDISTO D1\n\xa0has it completely covered with its impressive range of \n40m\n.\n\nDIMENSIONS:\xa011.5 x 4.35 x 2.35 cm\n\nIN STOCK\xa0\n\nThe \nDISTO D1\n is capable of more than just measuring. Speed up your workflow with the \nDISTO D1\n‘s integrated \nBluetooth\n functionality – for error-free measuring data transfer and documentation. \nBluetooth Smart Technology\n allows you to easily document and send data wirelessly from the work site to office.\n\nIt is possible to transfer measuring results direct to any smart phone or tablet. Pair your device with the\xa0\nDISTO D1\n and, using \nBluetooth® Smart data transfer\n,\xa0link to the \nFREE\xa0', 'The professional \nLT56 & LT58G\n\xa0\nint\ne\nrior measurement tools\n.\nThe\xa0\nLT56 & LT58G Laser Tools\n\xa0are the Go-To Interior Lasers. It provides 3 x 360° planes of bright red or green laser light that is ideally suited for all interior layout applications. The over-molded, tough housing is designed to withstand the rigors of the construction site and the compact design allows easy, secure mounting at ceiling height.\n\nPe\nr\nformance at a glance\n.\nThe LT58G contains a powerful rechargeable Lithium-ion battery that provides up to 25 continuous hours of green beam operation. It also can be operated directly with AC power. This eliminates the cost and waste of replacing alkaline batteries every day.\n\nThe unit is compact, lightweight and easy to mount. Installations on high ceiling grids will be a quick, easy task compared to conventional heavy rotating lasers and cumbersome mounts.\n\nMultiple Applications and Uses\n.\nFeatures & Benefits\nUltra-bright green laser technology\n – the industry’s brightest ', 'The 12V MAX* Green 3x360 Laser features 12V MAX* Lithium-ion battery and green beam laser technology. This laser is debris and water resistant with an IP65 rating and with an over-molded housing, it can withstand harsh conditions found on the worksite.\n\nFull-time pulse mode allows use with detector, maintains full brightness for visibility, and extends range\nOvermolded housing and IP65 debris/water resistance\nLocking pendulum helps prevent damage to internal components\n\nApplications:\n- Framing\n- Drywall\n- Extended Ceiling Bracket\n- Kitchen Installation\n- Interior Finishing\n- Layout\n- Plumbing Walls\n- Squaring Corners\n- LEVELING Walls to Foundation\n- Laying Steel track\n- Railing install\n- Laying Boards\n- Digging Footings\n- Retaining Wall\n- Patio\n- Tile Backsplash\n- Fireplace\n- Bathroom tile\n- Digging Consistent Depths\n- Laying Tile/Linoleum\n- Cuts outs\n- Level Countertops\n- Cabinet Install\n- Backsplash\n- Drywall Cutouts\n- Interior Can Lights\n- Use as baseline\n- Trim\n- Crown Molding\n\nInc', 'The Fluke 417D laser meter is accurate, durable, and easy to use—just point and shoot\nInstantly measure up to 40 m (131 ft.) with 1-button point-and-click\nContinuous measurement capable: adjusting as you move closer and farther from your target\nQuickly calculate area (sq feet/meters)\n1-meter drop tested and IP54 rated: built to withstand rainy or dusty conditions\nGreat for interior and exterior applications\n\nThe Fluke 417D is accurate, durable, and easy to use—just point and shoot. The simple design and easy, one-button measurement operation allows you to minimize time spent measuring and maximize the reliability of measurements.\nAdditional Product Features:\nLarge, 2-line illuminated LCD screen.\nThree different measurement tasks can be completed quickly and easily with one hand.\nThe bright laser is clearly visible, so you can always see your target point even from a hard-to-reach spot or long distance.\nDesigned for both indoor and outdoor applications.\nOperates with the Fluke durabilit', "New product\n\nShop\n\nLearn More\n\nItem\n #\nr9121031\n\nRobust laser meter with smart measuring functions and Bluetooth® connectivity for interior applications up to 100 m / 330 ft\n\n \n \n Measuring range:\xa0 2 in - 328 ft\n \n Measurement accuracy:\xa0 1.5 mm\n \n Measuring functions:\xa0 Single and continuous measurement\n \n \n\nFeatures\n\n\t    \t\t\t\n\t    \t\t\t\tRugged and durable housing – the laser measuring tool made for rough jobsite environments \n\t    \t\t\t\n\t    \t\t\n\n\t    \t\t\t\n\t    \t\t\t\tExtremely intuitive user interface with an ergonomic button design and layout \n\t    \t\t\t\n\t    \t\t\n\n\t    \t\t\t\n\t    \t\t\t\tCompact design to fit in every pocket \n\t    \t\t\t\n\t    \t\t\n\n\t    \t\t\t\n\t    \t\t\t\tExtra-long, integrated measuring extension spike to easily measure in narrow spaces, such as corners or window frames \n\t    \t\t\t\n\t    \t\t\n\nApplications\n\n\t    \t\t\t\n\t    \t\t\t\tDetermining the surface area of floors, walls and ceilings using the area or painter's area function \n\t    \t\t\t\n\t    \t\t\n\n\t    \t\t\t\n\t    \t\t\t\tVolume calculations for planning of hea", 'GLM 50 C Professional\n\nLaser Measures\n\nGLM 50 C Professional\n\nLaser Measures\n\n165 Ft. Laser Measure\n\nMeasuring distance extends to 165 Ft. with +/- 1/16 in. accuracy\n\nUpgraded color display with back lighting for increased visibility\n\nBluetooth® functionality\n\nBuilt-in inclinometer allows for advances features like angles, min/max, stake out and double indirect\n\nDefault real-time measurement shows how distances move in relation to the target\n\nFunctions include real-time length, length, area, volume and indirect\n\nHandy pocket-size design\n\nBack lighting allows users to see information in dark areas\n\nFree-to-download and use MeasureOn app - provides clear digital project overview, including floor plans, measurements, photos and notes\n\nBosch measuring and layout tools are covered by a one year limited warranty with an additional year when you register your tool within eight weeks of purchase - for details, visit https://rb-pt.io/PowerToolWarranty or call 1-877-BOSCH99\n\nGLM 50 C Professiona', 'Laser distance measures offer a fast and convenient solution to distance measuring applications that would otherwise require multiple steps to achieve. The Makita Laser Distance Measure, 262\' (model LD080P) is engineered to make tape measuring methods obsolete and provide unmatched productivity and sophistication for a full range of measuring applications. \nThe LD080P provides a distance operating range of up to 262\' for long distance capacity, and has a top-class accuracy of +/- 1/16" for maximum precision. For added versatility, it provides both standard and metric units of measurement, and the following measurement functions: Distance; Area; Volume; Permanent; Min/Max; Add/Subtract; Stake-Out; Pythagoras (2 point); Pythagoras (3 point); Pythagoras (partial height). Convenience features include an auto power-off function that shuts off the device automatically for increased run time performance, and a simplified user interface button and screen.\n\nFeatures\n\nMeasuring distance operatin']