["SKIL 10 AMP Fixed Base Router (RT1323-00)\n\nSpeed control dial provides the right speed for the material, and LED lights on the motor base illuminates the work area. Its ergonomic handles and tough die-cast motor housing makes this perfect for routing with both 1/2 in. and 1/4 in. shank router bits. The 10 Amp Fix Base Router's 1-3/4 HP motor cuts through soft and hard woods as well as plastic, and is also equipped with a live tool safety indicator, three LED lights, soft start with 6-speed variable control, quick-set screws for fixing the edge guide, and a built-in vacuum port.\n\nSKIL Router Table (SRT1039)\n\nCompatible with many major router brands, the SKIL SRT1039 Router Table brings convenience to the job. Get started with the quick and easy router clamp that attaches your router to the underside of the table. With the above table router lift, you'll get convenient access to adjust the height of the router bits without reaching underneath the table. This router table is also equipped", 'MRF23EVS Professional\n\nFixed-Base Routers\n\n2.3 HP Electronic Fixed-Base Router\n\nTrigger-control system – trigger power switch located in handle for enhanced control\n\nPowerful 15 Amp motor – produces 10,000 to 25,000 RPM and 2.3 horsepower\n\nPrecision-centering design – makes it easy to keep bit on cutline\n\nVersatile fixed-base depth adjustment – features 1-5/8 In. continuous microfine adjustment range\n\nAbove-table depth adjustment when fixed base is installed in router table\n\nConstant Response circuitry – maintains constant speed under load\n\nAlways-on LED lighting – for enhanced visibility in bit area\n\nSoft-start function – reduces start-up torque\n\nTwo-stage quick clamp system – for fast tool-free conversion\n\nVariable-speed dial – for matching speed to workpiece and task\n\nContoured soft grip handles – for enhanced control and comfort\n\nFixed base has threaded holes for mounting to router table positioned in common three-hole pattern\n\nCord swivel – for added mobility\n\nCompatible with opti', 'The MILWAUKEE® M18 FUEL™ Compact Router combines power, speed, and accurate depth adjustments to deliver clean accurate cuts in a variety of materials and applications. The compact router leverages the POWERSTATE™ Brushless Motor and REDLINK PLUS™ electronics. This delivers the power of corded 1.25 horsepower trim routers and best-in-class 31,000 RPM delivering users with power and speed for clean, quality cuts in hard materials. With an M18™ REDLITHIUM™ XC5.0 battery, the cordless compact router cuts up to 250ft of 3/8" roundovers in red-oak, providing users with all-day run time with fewer trips to the charger. The handheld router is equipped with a micro-adjust dial and macro-adjust button, giving users fast and accurate depth adjustments for precise work. A variable-speed dial with speeds from 10,000 to 31,000 RPM gives users control in all applications. The trim router also features a sturdy 4" sub-base plate giving users stability, and dual-LED lights illuminate their work surfac', 'The Rockwell 10pc. T-Shank Blade Set includes a variety of replacement blades for your BladeRunner X2. Cut wood, metal, tile, plastic and more! Order now.\n\nSwap these t-shank blades in and out of your BladeRunner in seconds, without the need for tools\nIncludes 10 blades for cutting metal, aluminum, ceramic and wood\nCompatible with the BladeRunner (RK7321) and BladeRunner X2 (RK7323)\nMultiple wood cutting blades allow you to choose between smooth or scroll cuts\nReplacement blades may be stored directly in your BladeRunner', 'The RIDGID 1-1/2 HP Compact Router features a soft start for gradual startup and extended motor life. With its variable speeds, you can easily adjust the router to your specific material type and application. With the micro adjust dial, you have more precise depth control.', 'The Makita 1-1/4 HP Compact Router (model RT0701C) delivers performance and precision in a compact design. With a full 1-1/4 maximum horsepower, the RT0701C is engineered for a range of precision routing applications. \nThe RT0701C has a powerful 1-1/4 HP (maximum horsepower) motor with a variable speed control dial (10,000-30,000 RPM) that enables the user to match the speed to the application. Additional performance features include electronic speed control to maintain constant speed under load, and soft start feature for smooth start-ups. The RT0701C is double-insulated with a heavy-duty aluminum motor housing for increased durability. \nThe RT0701C is engineered for precision and includes a smooth rack-and-pinion fine depth adjustment system and easy-to-read depth scales for more precise settings. The quick release cam lock system is designed for easy depth adjustments and base removal/installation, with a high-visibility base design for improved handling and performance. \nAdditional', 'Powerful 15-amp variable speed soft start motor provides speeds from 8,000 to 23,000 RPM\nPlunging base locks in downward position for functionality as both a plunge and a fixed router\nAccepts both 1/4 and 1/2-inch router bits with a plunge depth of up to 2-3/8 inches\n7-stop turret combined with both macro and micro-adjustment dials maximize precision\nIncludes a hard-shelled carrying case, a multi-function straight-edge fence, a template guide, a circle-cutting centering pin, a fence scale, a 1-1/2-inch dust collection duct, and a two-year warranty\nRemember when you had versatility and power all in the palm of your hand? Do you fancy chamfers and v-grooves or are you partial towards rabbets and dados? We won’t judge. That’ll just be between you and your router. Make intricate patterns in both the exterior and interior of your workpieces with the WEN 15-Amp Variable Speed Plunge Router. This versatile machine features a variable speed 15-amp motor, providing users speeds from 8,000 to 23']