Alfa Romeo V6 engine
Manufacturer | Alfa Romeo
Designer | Giuseppe Busso
Also called | Alfa Romeo V6 Busso
Production | 1979–2005
Block material | Aluminium
Head material | Aluminium
Valvetrain | SOHC/DOHC 60° 2/4 valves x cylinder, respectively
Turbocharger | Mitsubishi TD 05H (164) Garrett T25 (GTV,166)
Fuel system | 6 Dell'Orto carburetors Fuel injection
Management | Bosch L-Jetronic and Motronic
Fuel type | Petrol
Oil system | Wet sump
Cooling system | Water-cooled
Power output | 97–184 kW (132–250 PS)
Torque output | 178–300 N⋅m (131–221 lb⋅ft)
Predecessor | Alfa Romeo straight-6
Successor | JTS engine